Columbia University Academic Information Systems

Kermit News

Number 5, July 1993

This is not the real cover. The real cover shows a three-dimensional bar graph comparing XMODEM, YMODEM, ZMODEM, and Kermit file transfer for ASCII, Binary, and Precompressed files, on three different types of connections.

Contents

Editor’s Notes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

MS-DOS Kermit 3.13 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

C-Kermit 5A(189) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

IBM Mainframe Kermit-370 4.2.3–5 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

Other New Kermit Releases . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8

Kermit Distribution News . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 9

The Truth about Kermit File Transfer Performance . . . . . . . . . . . . . . . . . . 10 Long Packets and Sliding Windows . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10 Compression . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11 Prefixing . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11 Locking Shifts . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11 True-Life Benchmarks . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12

World News Kermit and the British Relief Mission to Bosnia . . . . . . . . . . . . . . . . . . . . . . . 15 Kermit in Germany . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 17 Kermit in China . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 19 Report from England: Kermit in Medical Research . . . . . . . . . . . . . . . . . . . . . . 20 Kermit in a Nonprofit Environment . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 22

Miscellany Modem Watch . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 23 Acknowledgements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 23

Kermit Software Distribution Ordering Information . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 24 Kermit Version List . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 25 Order Form . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 27

Kermit News (ISSN 0899-9309) is published periodically free of charge by Kermit Development and Distribution, Columbia University Academic Information Systems, 612 West 115th Street, New York, NY 10025, USA. Contributed articles are welcome.

Editor: Christine M. Gianone E-Mail: cmg@columbia.edu or kermit@cuvma.bitnet

Copyright © 1993, Trustees of Columbia University in the City of New York. Material in Kermit News may be quoted or reproduced in other publications without permission, but with proper attribution. And if you do, be sure to send us a copy!

The Kermit file transfer protocol is named after Kermit the Frog, star of the television series The Muppet Show, used by permission of Henson Associates, Inc.

Kermit News Number 5, July 1993 Page 1

Editor’s Notes

Welcome to Kermit News Number 5. This issue an- In countless cases, Kermit is chosen over other __ nounces new releases of MS-DOS Kermit for DOS alternatives ranging from public-domain and shareand Windows; C-Kermit for UNIX, OpenVMS, OS/2, ware packages, to expensive commercial software, to_{__} AOS/VS (and several other operating systems); and in-house development efforts because the quality is IBM Mainframe Kermit for VM/CMS, MVS/TSO, high and the cost is low. MUSIC, and now CICS. • If you are a vendor of modems, PCs, PC LANs, servers, laptops, notebooks, or palmtops, contact us The new generation of Kermit communications soft-_{__ __} about the benefits of and easy terms for bundling ware offers improved efficiency, networking capabil- MS-DOS Kermit software with your product. ities, automation features, and an understanding of • If you are a vendor of UNIX software and/or UNIXnational and international character sets. Together, based computers, ask us about bundling C-Kermit. __ the three major Kermit software programs MS-DOS_{__} • If you are a systems integrator, government contrac- Kermit, C-Kermit, and IBM Mainframe Kermit form tor, or vendor of any kind of computer hardware or a high-quality, powerful, and fully interopable suite software product or service, ask us how you can use of communication programs for the industry’s most Kermit software to lower your costs, improve your popular computers. operation, and get the edge on your competitors.

• If your organization is an end-user of computer hard- __ Credit Cards Accepted_{ware and software a corporation, a government}

agency, a hospital, a university or other nonprofit or We are also pleased to announce our new ability to_{__} public institution Kermit software can meet your accept Visa and MasterCard orders for Kermit soft- connectivity needs and stay within your budget. ware and documentation. This should simplify the ordering process for everyone. And if you are simply a private individual who wants

to communicate from home to office, to get online

It’s KermitWare! with commercial data services like MCI Mail or Com-

puServe, to hook up with BBSs, to transfer data ef- While Kermit software is not a commercial product, it ficiently and reliably between almost any conceivable is not in the public domain either, and never has pair of computers, Kermit software is for you!

been. It is not ‘‘shareware.’’ It’s not ‘‘freeware.’’ It is copyright by Columbia University. See page 24 for our terms and conditions.

As with any software, high-quality documentation is essential. It makes the user self-sufficient, it reduces the burden on the organizational help desk (and our Sprechen Sie Frangais? own!), and documentation sales help supply us with Using MS-DOS Kermit, second edition, has the income we need to continue our efforts. In this been translated into German by Gisbert W.

issue of Kermit News, I am pleased to announce the Selke, and published in Germany (see story, publication of a new edition of Using MS-DOS Kermit page 17):

and the new book, Using C-Kermit. Christine M. Gianone, MS-DOS Kermit, das universelle Kommunikationsprogramm,

Kermit Saves You Money_{Verlag Heinz Heise, Hannover (1991).}

In today’s economy, it has become increasingly impor- And into French by Jean Dutertre, and tant to obtain high quality at low cost. In ever- published in France: increasing numbers, government contractors are Christine M. Gianone, Kermit MS-DOS Mode proposing Kermit software and documentation in d’Emploi, Heinz Schiefer & Cie., Versailles (1993). their bids instead of commercial communication soft- And there is also a new Japanese book about ware. In the health care industry, Kermit software is MS-DOS Kermit: rapidly becoming the standard link from the doctor’s Hirofumi Fujii and Fukuko Yuasa, office, pharmacy, or hospital to the claims clearin- MS-Kermit Nyumon, Computer Today Library 6, ghouse or insurance company. Electronic claims sub- Saiensu-Sha Co., Ltd., Tokyo (1993). mission can speed the process and eliminate billions of dollars in paperwork each year.

Page 2 Number 5, July 1993 Kermit News

Announcing MS-DOS Kermit 3.13

MS-DOS Kermit is widely recognized as one of the Perhaps most important of all, now you can have a most powerful, efficient, and flexible of all PC com- single application program, a single configuration munication software packages for DOS and Microsoft file, and a common user interface for both serial and Windows. network communication.

While MS-DOS Kermit’s pricey competitors focus on Kermit’s TCP/IP and TELNET support works over frills like sound effects, elaborate startup screens, Ethernet- or SLIP-class packet drivers available from and technicolor pop-up exploding menus that con- your network board vendor or from us, as well as over sume your PC’s memory, disk, and processor ODI network drivers or on a serial port via Novell’s capacity, MS-DOS Kermit stresses substance: fast, new SLIP_PPP ODI driver, and also (via a ‘‘shim,’’ reliable, high-quality terminal emulation and file which we also supply) over NDIS drivers. transfer in a wide variety of communication, comput- Other Networks ing, and language environments. Small size and efficient operation. Easy setup and configuration. MS-DOS Kermit supports other networks too: AT&T Powerful, easy-to-use key mapping, macros, and StarLAN/StarGROUP, Digital Equipment Corporascript programming. And low cost. tion PATHWORKS (both LAT and CTERM protocols), IBM EBIOS/LANACS, NETBIOS, Intel OpenNET, Now MS-DOS Kermit extends its reach even further Novell NASI/NACS, Novell LAN Workplace for DOS with more terminal emulations, more communication TELAPI, InterConnections Inc. TES, 3Com BAPI, methods, faster file transfer, and more languages. and Ungermann-Bass Net/One, plus any BIOS Interrupt 14 interceptor for other network services, includ- Version 3.13 of MS-DOS Kermit for the IBM PC, ing external TCP/IP packages such as those from PS/2, and compatibles is now available. It was pre- Beame & Whiteside, FTP Software, or Wollongong. pared by Professor Joe R. Doupnik of the Center for Atmospheric and Space Sciences and Department of Compare MS-DOS Kermit with commercial PC com- Electrical Engineering of Utah State University in munication software packages. How many of them Logan, Utah, USA, in cooperation with Columbia support such a wide array of networks? And how University in New York City and Waterloo University many offer this support at no extra cost? in Ontario, Canada. Character Sets for Many Languages Built-in TCP/IP Networking Since version 3.0 was released in 1990, MS-DOS Ker- A major new feature of version 3.13 is its built-in sup- mit has been capable of preserving the national and port for TCP/IP networking, adapted from parts of international character sets used for Western Erick Engelke’s Waterloo TCP package and expanded European languages such as Italian, Norwegian, considerably to include TELNET protocol, multiple Portuguese, French, German, Spanish, Dutch, simultaneous sessions, and more. TCP/IP (Trans- Swedish, Danish, Finnish, and Icelandic during both mission Control Protocol / Internet Protocol) is the terminal emulation and file transfer. worldwide standard for open networking. Character-set conversion is essential in the inter- Why add TCP/IP to Kermit? Until now, people who national market. Different computers use different use both network and serial connections have had to encodings for the ‘‘special characters’’ found in these switch between a TCP/IP TELNET program (which languages; Kermit software can reconcile the difdoesn’t support serial connections) and Kermit (which ferences. didn’t support TELNET connections). No more! Now you you can use all of Kermit’s powerful features in Now MS-DOS Kermit also handles Eastern the TCP/IP environment in place of TELNET and FTP, European languages like Czech, Polish, Romanian, exactly as you use them now on serial connections: and Hungarian. And languages written in the script programming, modem dialing scripts (when Cyrillic alphabet such as Russian, Bulgarian, dialing out from TCP/IP terminal servers), flexible Byelorussian, and Ukrainian. It handles Hebrew key mapping, keyboard and command macros, fast too, including right-to-left screen writing and a full and accurate text and graphics terminal emulation, range of Hebrew VT100 and VT420 terminal feaand international character-set translation in both tures. MS-DOS Kermit 3.13 can even convert file transfer and terminal emulation. Japanese Kanji character sets during file transfer.

Kermit News Number 5, July 1993 Page 3

MS-DOS Kermit can transfer text files written in Modems and Dialing over 30 different languages with other computers, Kermit’s new dialing directory is a plain-text file even when they use completely different encodings, if that Kermit searches automatically whenever you the other computer is equipped with a Kermit pro- give a_{DIAL} command. Each entry contains a name, gram that uses this technique. IBM mainframe Ker- the associated phone number, the dialing speed, and mit and C-Kermit 5A do. This is a unique feature of the parity. It can be as long as you like. Here is a the Kermit file transfer protocol, and you won’t find it short (fictional) sample: in any other communications software.

sprintnet 7654321 2400 mark
tymnet 876-5432 1200 even

Terminal Emulation mcimail 987-6543 19200 none

compuserve 555-1212 9600 space

MS-DOS Kermit’s DEC VT terminal emulation is widely recognized as an industry leader: fast, ac- Just type ‘‘dial sprintnet’’ and Kermit does the rest:

curate, powerful, and full-featured. Now, thanks to a sets your speed and parity appropriately, commands development grant from Data General Corporation, your modem to place the call, and tells you (or your MS-DOS Kermit 3.13 adds Data General DASHER script program) whether the call succeeded or failed.

D463 and D470 text and graphics terminal emulations to its repertoire, suitable for use with DG’s As always, MS-DOS Kermit’s dialing is accomplished AOS/VS-based CEO system. Special capabilities invia script programs. In addition to the standard clude horizontal scrolling, compressed text, support Hayes script, new scripts are furnished for Telebit, for the DG International character set, and mouse US Robotics, Multitech, Penril, Practical Peripherals, support for CEO Draw. Supra, Vadic, and other modems, and for Rolm (Siemens) CBX data phones.

The new release includes other text and graphics terminal emulation improvements, too: 132-column For high-speed modems, MS-DOS Kermit now offers compressed text and horizontal scrolling in VT terbidirectional RTS/CTS hardware flow control, and minal emulation on EGA and VGA video adapters; a incorporates new defensive techniques required for compose key for entering accented letters; screen the new breed of low-cost high-speed internal rollback buffers and graphics images are now stored modems, and new controls for using them as COM3 or in expanded memory (EMS), if available, allowing

COM4 devices. 14400 bps is now supported as an in-

thousands of rollback screens while freeing conventerface speed, for use with V.32bis modems, and to tional memory for other uses. Terminal emulations comply with PTT regulations in many countries MSoffered by MS-DOS Kermit now include: DOS Kermit also now supports 75/1200 bps split- DEC VT52, VT100, VT102, VT220, VT320 speed operation.

DEC Sixel Color Graphics DG DASHER D463, D470 Text and Graphics Scripts and Macros Heath/Zenith 19 Tektronix 4014 Graphics with extensions Kermit’s script programming and macro features NONE (for external console drivers, e.g. ANSI) have been significantly extended. Macros can be longer. Command macros can now be assigned to Faster File Transfer keystrokes. Long variable names are allowed. New

built-in variables represent the current date, time, MS-DOS Kermit 3.13 includes important new file directory, etc. DOS files and environment variables transfer efficiency improvements. The limit on packcan be accessed by Kermit commands. And escape et buffers has been increased from 2K to 280K to atsequences sent by the host can run MS-DOS Kermit tain the theoretical maximum of 31 window slots of commands, for fully host-driven operation.

9024-byte packets for faster transfers on longdistance and network connections. Packet lengths New Documenation now adapt dynamically to noise conditions, and parity is detected automatically during packet opera- The user manual, Using MS-DOS Kermit, was uptions. For extra speed, selected control characters dated and a second edition published in 1992. It can be ‘‘unprefixed’’ during file transfer (see the ar- describes the new script programming and key mapticle on page 10). The file transfer display has been ping capabilities, and includes new character-set expanded and improved and, finally, a new capability tables, a new chapter on TCP/IP and other networks, has been added for transferring files with IBM main- a complete specification of the VT and Tektronix terframes through 3270 protocol converters that lack a minal emulators, and much more. Now available in transparent mode (see page 6). French and German (see page 1) as well as English.

Page 4 Number 5, July 1993 Kermit News

C-Kermit 5A(189) for UNIX, VMS, OS/2, AOS/VS, . . .

Quite possibly the world’s most portable communica- workstations to large enterprise mainframes, and oftion software package, C-Kermit 5A(189) for UNIX, fers all the capabilities of Kermit-32 plus all the new DEC VMS and OpenVMS, IBM OS/2, Data General capabilities of C-Kermit. AOS/VS, Apollo Aegis, MicroWare OS-9, the Commodore Amiga, and the Atari ST, offers: Unlike its predecessors, C-Kermit 5A has a comprehensive understanding of the VMS file system.

• Portability and consistency across hundreds of hard- When sending files, C-Kermit automatically selects ware and software platforms the appropriate mode, text or binary, based on each

• Efficient terminal connection and file transfer file’s record format. A new feature also allows more complex VMS files to be transferred in a way that • International appeal preserves all of their RMS attributes.

• Automation features

• Network support OS/2 C-Kermit

C-Kermit 5A is a full-function communications soft-

Portability ware package for OS/2 2.0 and 2.1 as well as for OS/2

1.3. In addition to all of C-Kermit’s regular features, The new C-Kermit release delivers high-quality comthe OS/2 version includes its own built-in VT102 termunications in all eight major operating systems it minal emulator complete with a sizeable screen, supports. It is distributed in C-language source code screen rollback, color control, printer control, key form and also in selected binary formats. It is availmapping, and other features familiar to users of MSable for computers ranging from desktop PCs and DOS Kermit. When run in an OS/2 window, Cworkstations to large central systems and supercom- Kermit also allows cutting and pasting, background puters. file transfer, and easy switching among applications. Early reports rate C-Kermit’s VT102 emulator among C-Kermit’s modular design has promoted its adapthe best available for OS/2.

tation to a diverse collection of computers and communication methods, making it a premiere example AOS/VS C-Kermit of open and portable software. C-Kermit’s user interface is easy to learn and use, helpful to the novice C-Kermit 5A is also available for Data General without getting in the way of the expert, and consis- Eclipse MV-Series minicomputers running AOS/VS tent throughout a wide range of operating systems and AOS/VS II. This full-featured C-Kermit version and hardware platforms. Users of many types of is already seeing heavy service at NASA (where, for computers now have a single software package to example, it is installed in the Spacelink information meet both serial and network communication needs. server) and the US Forest Service.

UNIX C-Kermit File Transfer Performance

C-Kermit 5A is available for the major UNIX Since its previous release, 4E(072) in 1989, C-Ker-variants, new and (within reason) old, including mit’s file transfer efficiency has been improved AT&T System III and V (R2, R3, R4), BSD (4.1–4.4 as dramatically by the addition of control-character well as 2.11), OSF/1, and POSIX, plus most popular ‘‘unprefixing,’’ sliding windows (up to 31 window commercial UNIX products, including AIX, A/UX, slots), and long packets (up to 9024 bytes), bringing BSDI, DG/UX, DNIX, DYNIX, DYNIX/PTX, DRS/NX,_{__} file transfer efficiency even over long-delay satellite ESIX, HP-UX, IRIX, NeXTSTEP, QNX, SCO (XENIX,_{__} and/or public network connections into the 95%– UNIX, and ODT), Solaris, SunOS, ULTRIX, UMAX, 100% range, or better, with excellent error recovery UMIPS, UNIPLUS, UnixWare, UNOS, and many characteristics on noisy connections.

more (see our version list on page 25).

The sliding window transport, perfected over three VMS C-Kermit years of field testing, uses selective retransmission to Users of DEC (Open)VMS can bid a fond farewell to minimize overhead on noisy connections, and the Kermit-32. Support disappeared years ago, never to packet length adapts automatically to noise characbe fully replaced because Kermit-32 is written in a teristics. Errors are detected by 16-bit CRC and language (Bliss) found at very few sites. C-Kermit 5A other methods. For more about efficiency, plus realis available for both VAX and Alpha AXP versions of life benchmarks comparing Kermit with other proto- (Open)VMS, on processors ranging from desktop cols, see the article on page 10.

Kermit News Number 5, July 1993 Page 5

International Appeal Communication Features

The Kermit protocol stands alone in its ability to con- Dialing is accomplished with C-Kermit’s expanded vert a file’s character set during transfer in a mixed built-in support for a wide variety of modems, plus a computing environment. For example, an Italian- new text-based dialing directory compatible with MSlanguage document written in Code Page 437 on a PC DOS Kermit’s, and an even more powerful text-based is correctly translated during transmsission to (say) a services directory that not only establishes your con- DEC workstation using the DEC Multinational Char- nection but also logs you in automatically. The OS/2 acter Set. Despite their differing internal represen- and many of the UNIX C-Kermit versions (depending tations, the accented letters come out the same on on the capabilities of the underlying operating sysboth ends, rather than the gibberish often seen when tem) also support hardware flow control for use with transmitting such text across vendor, language, or terminal servers and high-speed modems. character-set boundaries. C-Kermit 5A supports not only serial (direct and C-Kermit’s character-set conversion capabilities are dialed) connections, but also TCP/IP connections in not confined to West-European languages like most UNIX versions, in the AOS/VS version, in the Italian, French, German, Spanish, Norwegian, and OS/2 version, and also for VMS systems equipped Portuguese, but also extend to East-European lan- with DEC TCP/IP (UCX), TGV MultiNet, Wollongong guages like Hungarian, Czech, Polish, and Romanian, WIN/TCP or PathWay, or with Process Software as well as to languages written in the Cyrillic al- TCPware. phabet, like Russian and Ukrainian, and also to Hebrew and to Japanese Kanji. On Sun computers equipped with SunLink X.25, C- Kermit 5A also supports X.25 connections. And on Most of the same conversions are also available dur- OS/2 systems equipped with DEC PATHWORKS, Cing terminal connection, screen capture, and ‘‘ASCII Kermit can make DECnet LAT connections. upload’’, and can also be used to change a local file’s character-set ‘‘in place’’. Language-specific rules (e.g. On TCP/IP networks, C-Kermit can be used in place ‘‘c’’ to ‘‘ae’’) can be applied when translating text writ- of TELNET and FTP with several advantages. Cten in languages like German, Dutch, Swedish, or Kermit’s TELNET connections handle character-set French into ASCII. conversion, key mapping and macros, session logging, and other functions lacking from normal TELNET soft- __ In the 7-bit communication environment an area ware. C-Kermit’s DIAL command command can be __ neglected or ignored by most other protocols efficient used to place calls using modems that are connected transfer of 8-bit textual data (such as Cyrillic or to network-accessible reverse terminal servers. Kanji) is achieved using a new locking-shift mechanism, discussed on pages 11 and 14. Kermit file transfer offers features lacking from FTP: correct handling of file size and date, character-set The advanced Kermit protocol features of C-Kermit conversion, an update feature, numerous options for 5A can be used to full advantage with MS-DOS Ker- handling filename collisions, convenient methods of mit on PCs with DOS or Windows, IBM Mainframe transfer interruption, and so on. And, unlike tradi- Kermit-370 for VM/CMS, MVS/TSO, or CICS, and, of tional TELNET and FTP programs, C-Kermit’s network course, with another copy of C-Kermit 5A itself on operations can be fully automated. UNIX, VMS, OS/2, AOS/VS, or any of the other operating systems where it runs. Documentation

C-Kermit 5A comes with the new Digital Press book,

Automation Features Using C-Kermit, by Frank da Cruz (author of Kermit,

C-Kermit’s automation features include key mapping A File Transfer Protocol) and Christine M. Gianone and keystroke macros for use during terminal connec- (author of Using MS-DOS Kermit), which is geared tion, plus command and initialization files, command towards both the beginner and the expert. The book macros, and a fully functional script programming includes tutorials, numerous illustrations and tables, language. Any kind of routine communication task hundreds of examples, as well as easy-to-use and can be fully automated, from connection establish- comprehensive reference features. ment, to logging in, to interacting with a remote host or service, to file transfer, to logging out and connec- A German-language edition, C-Kermit, Einfyhrung tion release. C-Kermit’s script language is almost und Referenz, will be available in October from Verfully compatible with MS-DOS Kermit’s, and script lag Heinz Heise in Hannover, Germany (see article on programs can be written that work with both. page 17).

Page 6 Number 5, July 1993 Kermit News

IBM Mainframe Kermit-370 for VM/CMS, MVS/TSO, CICS

John F. Chandler Harvard/Smithsonian Center for Astrophysics Cambridge, Massachusetts

proved support for Generation Data Groups in TSO, There have been several new releases of IBM mainand improved installation procedures.

frame Kermit-370 since version 4.2 was announced in the last issue of Kermit News. Most notable among • Support for a new method of Kermit file transfer through 3270 protocol emulators, such as the 3708, these is a brand-new version for CICS, which can be that do not offer transparent mode.

used under either MVS or DOS/VSE. The new releases run on all the major operating systems found CICS Kermit is already serving diverse applications:

on the IBM System/370 (390, 9000) architecture, including XA and ESA: • The CICS-based NOTIS bibliographic database system has been equipped with a mechanism for CICS Kermit 4.2.4 downloading search results with Kermit.

For CICS versions 1.6–2.1 under MVS, DOS/VSE, and probably also VM (this has not yet been • Washington University has a CICS-resident e-mail tested), supporting the full range of linemode and system that receives electronic mail messages from fullscreen environments that are supported by the the PC via Kermit. Other forms of special-purpose other Kermit-370 versions. uploads and downloads with Kermit acting as a ‘‘subroutine’’ are also in use.

TSO Kermit 4.2.4 • The library of the University of New Brunswick has For MVS/TSO, MVS/XA/TSO, and an automated circulation system implemented under MVS/ROSCOE/ETSO. CICS. Each location has at least one PC signed on to CMS Kermit 4.2.5 the system. When the mainframe is down, trans- For VM/CMS, VM/ESA/CMS, VM/XA/CMS, actions are recorded on the PC and uploaded and ap- VM/HPO/CMS, VM/IS/CMS, and VM/SP3–SP6. plied when the mainframe comes back up.

MUSIC Kermit 4.2.3 • Miami University has a network that collects data by For the MUSIC/SP operating system, with MUSIC day for nightly retrieval. The collection is automatispecifics by Pierre Goyette of McGill University. cally uploaded using Kermit-CICS.

Major new features include:

3270 Protocol Converters

• Support for more communication environments and IBM 370 and compatible mainframes generally supfront ends, notably the IBM 3174 AEA B2.0. Support port both linemode (TTY) and fullscreen (3270) sesfor 8-bit no-parity file transfer through front ends sions. Both are marked by the need for communithat support it, and automatic detection of a wider cations front ends that variously translate between variety of front ends and 3270 protocol converters. EBCDIC and ASCII and try to make ASCII terminals • Support for more character sets. In addition to the look like IBM terminals.

ISO-based Roman, Cyrillic, Greek, Hebrew, and Japanese Katakana character sets supported by version 4.2, the new releases also support Latin-2 and Linemode connections generally do not pose a serious Latin-3 based character sets for the East European problem for Kermit file transfer; Kermit needs only to Roman-alphabet languages, and full Japanese Kanji. undo the front end’s ASCII/EBCDIC translation by Kermit-370 now supports character-set conversion for performing reverse translations in each direction. the following languages: Afrikaans, Albanian, Fullscreen connections, however, go through 3270 Basque, Breton, Bulgarian, Byelorussian, Catalan, protocol converters that perform complicated func- Croatian, Czech, Danish, Dutch, English, Esperanto, tions like screen formatting and optimization that in- Faeroese, Finnish, French, Frisian, Gaelic, Galician, terfere with Kermit packets. Many, but not all, 3270 German, Greek, Hebrew, Hungarian, Icelandic, Italian, Japanese (both Katakana and Kanji), Latin, protocol converters offer a transparent mode that can Macedonian, Maltese, Norwegian, Polish, Portuguese, be used to disable these functions, allowing Kermit Quechua, Rhaetian, Romanian, Russian, Serbian, packets to pass through without modification. Slovak, Slovenian, Spanish, Swahili, Swedish, Turkish, Ukrainian, and Volapuk. The welter of competing and often incompatible com-

• Support for the new Kermit protocol locking-shift munications devices would cause a major headache mechanism (see page 11). for the poor Kermit user, except for three circum-

• Better recovery from communication I/O errors, im- stances. First, Kermit-370 has routines to automatiproved on-line help, carriage-control conversion, im- cally detect which kind of front end is controlling the

Kermit News Number 5, July 1993 Page 7

current session; second, the Kermit installer is en- Kermit-370’s new FULLSCREEN mode has changed all couraged to tailor Kermit to force the correct SET that. The SET CONTROLLER FULLSCREEN command al-

CONTROLLER default whenever those routines don’t lows file transfer with no control characters at all

work properly; and, third, Kermit now offers a last- and, therefore, without a transparent mode when resort mode of operation that will work with protocol used with a suitable transfer partner: converters that do not include a transparent mode. • It allows Kermit packets to start with a printable character rather than a control character.

What Is Transparent Mode?_{• It frames the packet by its length field rather than}

Transparent (sometimes known as ‘‘graphics’’) mode depending on a ‘‘line terminator.’’ is a special type of operation in a protocol converter • It ensures there are no strings of repeated blanks in that passes the inbound and outbound data streams the Kermit packets. straight through (but modifying the parity in many • It ensures that the Kermit packet does not end with cases), devised largely to allow interactive graphics a blank. on non-IBM graphics terminals. • It restricts the packet length to fit within the screen width to prevent ‘‘wraparound’’ by the protocol con- Graphics applications need to transmit escape se- verter. quences or other control characters back and forth between the mainframe and the terminal, but a protocol Kermit programs that need to transfer files with Kerconverter normally filters out all control characters in mit-370 in fullscreen mode must be modified to acboth directions. In practice, the normal Kermit proto- count for these factors, and also must be prepared to col needs just one transmittable control character for ignore reflections of their own packets, which are each direction to synchronize the encoding and decod- echoed back once by the protocol converter and someing of packets. times again by the operating system.

Although protocol converters are advertised as Kermit-370, MS-DOS Kermit 3.13, and C-Kermit 5A simulating the behavior of IBM 3270-type terminals, incorporate the needed modifications, and successful they offer several different approaches to trans-_{FULLSCREEN} transfers are reported through pre-B2 parency. The device and Kermit must agree on the IBM AEA controllers, the IBM 3708, Micom 7400, method; the SET CONTROLLER command can be used Sim3278/VTAM, and various tn3270 implementato force a particular style of transparent mode. Here tions, including those found in terminal servers from are Kermit-370’s SET CONTROLLER options, listing the Xyplex and others. devices they are known (or reported) to work with:

Use FULLSCREEN mode only as a last resort: the re- TTY quirement for short packets and the time needed to (Linemode) Amdahl 4705; IBM 37x5, 3708, or absorb multiply echoed packets reduce efficiency, and 8232; Comten 36xx; STNxx; Jupiter 1000; K200, the lack of a unique packet synchronization character K310, or K2000. complicates error recovery procedures on noisy con- SERIES1 nections.

Yale ASCII system on IBM Series/1 or 4994; IBM 7171 or 937x ASCII subsystem; Hydra II; Comm- To set up a FULLSCREEN mode file transfer, issue the tex Cx-80; SIM3278/TCPIP 2.0 or /VM 5.0; tn3270; following commands:

Cisco 516-CS.

C-Kermit or GRAPHICS Kermit-370 MS-DOS Kermit Datalynx 3174 or 3274; Datastar 4025; Data-

SET CONTROLLER FULL

stream/Leedata 8010, 8030, or 874; PCI 1076 or

SET RECEIVE START 62 SET SEND START 62

276; Renex PCM, TMS-x, RPAD, or RTD; KMW

SET SEND START 62 SET RECEIVE START 62

S/II 3270.

SET BLOCK B SET BLOCK B

AEA

SET HANDSHAKE 0 SET HANDSHAKE NONE

IBM 3174 AEA (B2 or higher).

This sets the packet-start character in both directions FULLSCREEN-Mode File Transfer to be the greater-than sign (>) (ASCII 62) and enables

a new block-check type (a 12-bit checksum containing What if your 3270 protocol converter is not supported no blanks) to defeat the trailing-blank-stripping feaby one of the SET CONTROLLER commands listed ture found in many protocol converters. Short packabove? Until now, Kermit file transfer through such ets are used automatically.

devices was not possible.

Page 8 Number 5, July 1993 Kermit News

Support was added for the Microbee family of com-

Other New Kermit Releases_{puters (56K, 64K, 128K and 256K) manufactured by}

Microbee Systems, Ltd, of Australia, by Russell Lang Acorn Archimedes Kermit of Monash University, Australia, and for the Ampro Little Board from Jay S. Rouman of Mt. Pleasant, MI, From Cosmos Nicolaou and Andrew Brooks, via Lan- USA. April 1991. Tape A.

caster University in the UK, Kermit for the Acorn Archimedes with the RISC_OS operating system, a port DEC PDP-8 and PDP-12 of the ACW Panos version. May 1993. Tape C. From Charles Lasner. Bug fixes and a new encoding Apple II Kermit 3.87 format for bootstrapping this program to your PDP-8 or PDP-12. September 1990. Tape D.

From Ted Medin. New features include: screen restore on CONNECT for Apple IIe or later models; Ker- Gould/SEL MPX Kermit 2.3 mit file attributes are now handled; percent of file From Barry M. Wilson, Queensland Electricity Comtransferred shown when possible (file attributes remision, Australia: a new Kermit server program for quired); a new driver for the Ace dual card. Also, the Gould/SEL 32/77 computer with the MPX 1.5E many bugs fixed, terminal emulation and printer supoperating system. It supports long packets and port improved. December 1990. Tape A. handles run-length compression in incoming packets.

BTOS / CTOS Kermit 2.00 November 1990. Tape D.

From Evan Arnerich and Doug Drury of ITT Federal Hewlett Packard 3000 MPE Kermit Services Corporation, Santa Maria, CA: version 2.00 From Tony Appelget, General Mills, Inc., Minof CT-Kermit for the Burroughs B20/BTOS and Conneapolis, MN. New features of this version, written vergent NGEN/CTOS systems. in the SPL language, include long packets, support for 16-bit CRC error checking, improved operation This new version adds some of the capabilities of MSwith HP Spectrum machines, a versatile command DOS Kermit 3.x and C-Kermit 5A, particularly script abbreviation scheme, a new HELP function, and many programming features (INPUT, OUTPUT, IF, ASK, GOTO, bug fixes. October 1991. Tape D.

variables, etc), and includes a built-in VT101 terminal emulator. January 1993. Tape C. A second version of the same program, but written in Chinese DOS Kermit the C language, was received from Tony in June 1993. Tape D.

An adaptation of MS-DOS Kermit 2.32/A to CC-DOS, the Chinese version of MS-DOS, also known as Honeywell DPS-6 Kermit 2.01 LIANXIAN, STCDOS, CCDOS213, and GWCDOS, From Frank Dreano, Chesapeake, VA. New features written by Quanfang Zhang of Zhezhiang University, of version 2.01 include wildcard sends; REMOTE com- Hangzhou, China. See the article on page 19. mands for servers; ability to transfer foreign binary Commodore 64/128 Kermit files both ways; bug fixes. June 1991. Tape D.

Updated to include support for the Swiftlink-232 IBM CS-9000 Kermit serial interface by Kent Sullivan, Matthew Sorrels, For the circa-1980 IBM laboratory workstation, a and Ray Moody. September 1992. Tape C. send-only Kermit program (so you can get your files CP/M-80 Kermit 4.11 off it) from Glenn Howes, University of Wisconsin, written in Pascal. September 1992. Tape C.

From Mike Freeman, Bonneville Power Administration, Vancouver, WA, USA. Luxor Computers

Furnished by Bo Kullmar, chairperson, ABC-Klub- Features added since version 4.09 (January 1988) inben, Stockholm, Sweden.

clude: new filename collision options: BACKUP,

DISCARD, OVERWRITE, RENAME; an option to keep or

Protocol fixes for ABC80 and ABC800 from Jsrgen discard incompletely received files; many new Westman of ABC-Klubben. ABC800/802/806 CP/M

REMOTE commands for communicating with Kermit

systems updated to version 4.11, with support added servers; a RENAME command; improved interruption for FACIT DTC and DTC2 Luxor clones, from Mikael of TAKE, TYPE, and PRINT commands in progress; Johansson of ABC-Klubben. July 1990. Tape C.

many bug fixes.

Kermit News Number 5, July 1993 Page 9

NCR 9800 VE/IVS and VE/MCS Kermit Distribution News

From Paul E. Gladden of NCR Corporation, San Diego, California, USA: a new Kermit program for Max Evarts, Kermit Distribution Columbia University, New York City the NCR 9800-4 computer with the NCR VE4.0 operating system. The Kermit Distribution and Support office has seen many changes since the last issue of Kermit News. In Separate variations are provided for the IVS and June 1990 Ken Suh moved on to law school and Andy MCS environments. The program is written in C, Newcomb took his place. Many of you who have based on C-Kermit 4E with features selected dependcalled us over the past few years already know Andy.

ing on VRX system capabilities. July 1990. Tape D.

Pecan Kermit 1.1 New Services

From R. Tim Coslet. Atari Mega ST2 under Pecan We can now accept credit card orders by phone. We Software Systems UCSD p-System Version IV.2.2 can also accept credit card orders and purchase orwith Standard File System (SFS). ders by fax. With our optional rush service, you can have your Kermit software within 24 hours! (Rush Binary transfers now work in both SFS and AFS im- orders received after 4:00 PM New York time ship the plementations. Incorrect reporting of file creation next day.) See the order form for details. time in attribute packet fixed. July 1990. Tape C. In response to the growing demand for telephone ser- Prime Kermit 8.15 vice, we are putting in a call-processing system. If all

From John Horne Polytechnic South West, Plymouth, lines are busy, you will have options to get the infor- U.K., with contributions from Matthew Sutter: a new mation you need from our voice menu or hold to release of Prime Kermit that can initiate outbound speak to one of us. The system separates orderconnections. There is a new CONNECT command, with related calls and technical calls so those of you with a accompanying features for logging a terminal session, quick ordering question will not have to wait while setting the transmission speed, duplex, and the we debug a software problem.

CONNECT-mode escape character, plus a selection of CONNECT-mode escape functions. Technical Support Hints

Speaking of phones and Kermit problems, Andy and I Other new features include: ability to send BYE, now handle a substantial percentage of the technical

FINISH, SEND, GET, and selected REMOTE commands to

support calls that come in. Here are a few pointers Kermit servers; script programming features, includfor those calling in for tech support:

ing new INPUT, OUTPUT, PAUSE, and CLEAR commands; problems with multiple file transfers with a specific • Make sure you have the current documentation for file type are corrected. your Kermit software; if we are on the phone reading the manual to you, we cannot be helping someone There are also improvements in sliding windows and who has a more difficult Kermit problem. other Kermit file transfer protocol features; the exact • Know the versions of all the Kermit programs infile length is now sent in the attributes packet; an volved before you call; most Kermit programs print alternate initialization filename is specifiable on the the version number when they start up. command line; pound-sign conversion is correctly • Expect us to ask you to upgrade your Kermit software handled. April 1993. Tape D. if you are far behind the times; we can only support up-to-date versions.

TurboDOS Kermit • Try to be in a position where you can reproduce your

From Mark Eichen at MIT. This one was written problem while you are on the phone. years ago, an adaptation of an earlier release of • We do not support implementations of the Kermit file CP/M-80 Kermit. The source code was lost. The bi- transfer protocol that are part of other communicanary executable program is available in hex form. tions packages. October 1992. Tape C. Our technical support service is a free, but limited, UNISYS (Burroughs) A-Series Kermit 1.041 resource. Usually, only one person is available at a time to handle tech support calls; please be con- From Dave Squire, Computing Services, University of_{__} siderate of the many other callers help us to help as California at Davis. Long packets, alternate block many Kermit users as we can.

checks, command files. July 1990. Tape D.

Page 10 Number 5, July 1993 Kermit News

The Truth about Kermit File Transfer Performance

Frank da Cruz

In the early 1980s, the first generation of Kermit soft- packet plus the 2-second delay make 5 seconds, so ware used the basic Kermit protocol: stop-and-wait throughput is 180 bps, 60% efficiency. At 9600 bps, it exchange of short packets. The basic protocol is takes only 1/10 second to transmit the same packet, easily implemented and highly robust, and led to its but the delay is still 2 seconds. Throughput is only rapid proliferation to hundreds of hardware and soft- 428 bps, 4.5% efficiency. When connections have ware platforms where it proved a success in trans- delays, efficiency can be improved by lengthening the ferring files under even the most difficult conditions. packets, but only if the connection is clean. On a noisy connection, longer packets are more likely to be damaged in transmission and take longer to re- The new generation of Kermit software improves on transmit.

the original robust qualities and dramatically boosts performance without sacrificing compatibility with the earlier generation. Protocol capabilities are nego- On full-duplex connections, the new generation of tiated automatically so the newest, most advanced Kermit software (IBM mainframe Kermit excluded, versions can still exchange files with the earliest or which always has a half-duplex connection) can most minimal versions. transmit packets in a steady stream, processing the acknowledgements later as they arrive, thus eliminating the effects of transmission delays, and also Kermit’s performance features include long packets, eliminating the overhead of the acknowledgements sliding windows, control-prefixing selection, locking themselves, since they are ‘‘on the wire’’ at the same shifts, and compression. The first three have the time as the data packets and therefore don’t take up potential for causing problems, and are not used unany extra transmission time. This technique is called less you ask for them. This article describes Kermit’s sliding windows, because multiple packets are kept performance features and tests them against other in a buffer (window) that ‘‘slides’’ forward whenever popular protocols. The results might surprise you. the oldest packet in the window is acknowledged.

Long Packets and Sliding Windows

Using 94-byte packets without sliding windows on a The maximum packet length in the basic Kermit pro- connection that has a 1-second delay results (accordtocol is 94, chosen to prevent data loss when the ing to actual measurements) in an efficiency of about receiver has small input buffers or lacks an adequate 8%. Raising the packet length to 1500 on the same method of flow control, and also to reduce vul- connection increases the efficiency to 63%. Using nerability to noise. But since 1985, Kermit’s long- sliding windows on the same connection raises the efpacket extension has allowed packets up to 9024 ficiency to 82–90%, depending on the packet length. bytes in length to be used when conditions permit.

Optimum performance can be achieved on Longer packets reduce the ratio of protocol overhead any given connection by choosing the to actual data, increasing the potential file transfer right combination of packet length and efficiency (the ratio of file characters transferred per window size.

second to the actual connection speed) from 86% (for 94-byte packets) to 95% (with 2500-byte packets). When conditions deteriorate on the connection, the To see a dramatic speed improvement using MS-DOS packet length is automatically adjusted. Kermit 3.13 and/or C-Kermit 5A, simply give these

commands to each Kermit before file transfer: Original, basic Kermit was a stop-and-wait protocol

SET WINDOW 3

because it had to work on half-duplex as well as full- SET RECEIVE PACKET-LENGTH 1000 duplex connections. But connections through satel- Adjust as necessary. Longer delays require larger lites or packet-switched networks can have delays windows; noisier connections (or devices with small that seriously impede the efficiency of a stop-and-input buffers) need shorter packets. MS-DOS Kermit wait packet protocol. For example, suppose packets 3.13 and most versions of C-Kermit 5A allow the are 90 bytes = 900 bits long, and there is a one-second theoretical maximum sizes, 31 and 9024 respectively, transmission delay. For one packet and its response, sufficient to overcome any reasonable delay (for exthe round-trip delay is 2 seconds. At 300 bits per ample, between the earth and the moon).

second (bps), the 3 seconds required to transmit the

Kermit News Number 5, July 1993 Page 11

On 8-bit connections, Kermit transfers 8-bit data

Compression

with no additional overhead. On 7-bit connections, To reduce transmission overhead, the Kermit protocol_{__} which are quite common these are the connections uses a simple, but often surprisingly effective, com- that use even, odd, mark, or space parity, often with-

pression technique: repeated byte values are repre-_{__} out the user’s knowledge 8-bit data is encoded using sented by a count+byte combination. This technique a single-shift technique, a prefix character for each

is easy to program and inexpensive in memory and byte whose 8th bit is 1, similar to holding down the

CPU cycles, and is therefore implemented in most

Kermit software, including MS-DOS Kermit, C-

The Kermit protocol implementations Kermit, and IBM mainframe Kermit, and is used

found in many of the popular commercial automatically when available.

and shareware PC communication soft-

ware packages are minimal and per- Analysis of large volumes of both textual and binary

functory, usually lacking some or all of data shows an average compression of 15–20%.

the performance features . . . Dramatic savings are achieved in certain types of

files, including tabular text (or any other type of text

with lots of repeated characters) and executable pro- Shift key on your keyboard for each 8-bit character.

grams containing large amounts of pre-zeroed data. This allows Kermit to work where most other protocols

fail. The amount of prefixing ranges from 0% up to

Prefixing 100%, depending on the type of file.

To achieve its ability to push data through even the_{__}

most restrictive types of connections for example, to Locking Shifts

mainframes that are sensitive to certain control char- To avoid the high overhead of transferring 8-bit text, acters, or on 7-bit connections, or on very noisy ones particulary Cyrillic, Hebrew, or Kanji, on 7-bit con- (one user said recently, ‘‘Kermit will send data over a nections, a new ‘‘locking-shift’’ feature works like the communication channel that is only slightly better Caps Lock key on your PC: a special shift prefix ap- __ than a pair of tin cans connected with a wet string’’) plies to a entire run of 8-bit characters, no matter Kermit formats its packets as lines of printable text. how long, rather than to a single character. Locking This is done by encoding each control character as a shifts are used in combination with single shifts to sequence of two printable characters and, on 7-bit achieve the most compact encoding.

connections only, encoding 8-bit characters as a se-

quence of two printable 7-bit bytes. Locking shifts are supported by MS-DOS Kermit

3.13, C-Kermit 5A, and IBM Mainframe Kermit 4.2.4, On some connections it is safe to transmit certain and are negotiated automatically when parity is in control characters ‘‘bare,’’ without prefixing or encoduse (including when parity is detected automatically).

ing. ‘‘Unprefixing’’ of control characters can speed up They reduce the 8th-bit prefixing penalty anywhere the transfer of binary files, particularly precomfrom 0% to 100%, depending on the groupings of the pressed files, which tend to contain a lot of bytes in 8-bit characters within the file.

the control range. MS-DOS Kermit 3.13 and C-

Kermit 5A(189) give you the ability to specify which

So Why the Bad Reputation?

control characters are to be prefixed and which are

not. In the benchmarks on pages 12 and 13, only The Kermit protocol implementations found in many

three control characters are prefixed: of the popular commercial and shareware PC com-

SET CONTROL UNPREFIXED ALL munication software packages are minimal and per-

SET CONTROL PREFIXED 0 1 129 functory, usually lacking some or all of the perfor-

mance features just described. Many of these same This technique can be used even if the Kermit pro-

packages also include XMODEM, YMODEM, or gram on the other end doesn’t know anything about

ZMODEM protocol, which (when they work at all) it, since well-designed Kermit software will, indeed,

usually perform better than the basic short-packet, accept bare control characters literally. The three ex-

stop-and-wait, prefix-everything Kermit protocol. ceptions above are NUL (0), which is used internally

Using a limited Kermit implementation is like filling by C-Kermit for string termination, and SOH (1) and

your bathtup from a dripping faucet instead of turn- SOH+parity (129), Kermit’s normal packet-start in-

ing the water on full blast. It is easy to see why users dicator. It takes some experimentation to find the

of such packages might conclude that Kermit file maximum safe set. That’s why Kermit prefixes all

transfers are slow. Nothing could be further from control characters by default: first make it work, then

truth; turn the page and see for yourself. make it fast.

Page 12 Number 5, July 1993 Kermit News

True-Life Benchmarks

Table 1 illustrates the performance of the Kermit protocol implementations found in different PC software packages. These measurements were made on a direct 19200-bps serial connection, downloading a typical ASCII text file (the VM/CMS Kermit-370 manual), 135087 bytes in length, from a Sun SPARCserver-10 with C-Kermit 5A(189) to the hard disk of an IBM PS/2 Model 70.

Table 1 Kermit Implementations Compared

Window Packet Time Speed PC Software Size Length (secs) (cps) Efficiency Remarks

Telix 1 94 131 1052 55% Long packets and sliding windows not available MTEZ 1 94 119 1158 60% Long packets and sliding windows not available Smartcom III 1 94 113 1220 64% Long packets and sliding windows not available PROCOMM PLUS 14 1000 77 1790 93% Window size not selectable Zstem 340 2 1000 74 1863 97% Maximum window size is 2 MS-DOS Kermit 3 1000 72 1915 99% Full control-character prefixing MS-DOS Kermit 3 1000 69 1999 104% Only 0, 1, and 129 prefixed

The results speak for themselves.

If you thought Kermit file transfer was slow, you were probably not using real Kermit software!

The UNIX-resident copy of the file, like all UNIX text files, uses only linefeed (LF) for line termination. During text-mode transfer, each LF becomes carriage return and linefeed (CRLF). There are 2814 lines in the file, so the actual data size during (and after) transfer is 137901. Since the connection runs at 1920 characters per second (10 bits per character), a 100%-efficiency transfer should take 137901 / 1920 = 71.8 seconds. The following PC communications software was used:

MS-DOS Kermit 3.13 Columbia University, New York, NY, USA MTEZ 1.16 MagicSoft, Inc., Lombard, IL, USA PROCOMM PLUS 2.0 Datastorm Technologies, Inc., Columbia, MO, USA Smartcom III 1.0A Hayes Microcomputer Products, Inc, Norcross, GA, USA Telix 3.21 deltaComm Development, Cary, NC, USA Zstem 340 1.0.4 KEA Systems Ltd., Burnaby, BC, Canada

Kermit and X-Y-ZMODEM

XMODEM, YMODEM, and ZMODEM are the file tranfer protocols most commonly compared with Kermit, and which are found in numerous shareware and commercial communication software packages. XMODEM and YMODEM are stop-and-wait protocols; XMODEM uses short blocks (128 data bytes), YMODEM uses longer ones (1024 data bytes). ZMODEM is a streaming protocol.

The tables on page 13 compare XMODEM, YMODEM, ZMODEM, and Kermit transfers between the PC and UNIX. The file transfer software on the UNIX system is sx (XMODEM) / sb (YMODEM) / sz (ZMODEM) 3.24 (June 1993) and C-Kermit 5A(189). On the PC, X-, Y- and ZMODEM transfers were done with Telix and PROCOMM PLUS (which gave exactly the same results). For fairness, four types of files are transferred:

ASCII Text: IKCKER.DOC 137901 bytes Our original ASCII text file, text mode UNIX Binary: uuencode 24576 bytes A Sun SPARC binary executable program, binary mode PC Binary: KERMIT.EXE 197928 bytes An MS-DOS binary executable program, binary mode Precompressed: KERMIT.ZIP 238584 bytes A compressed ZIP archive,binary mode

Tests were performed on four types of connections and in each trial, Kermit transfers used a window size of 5 and a packet length of 5000, and control prefixing was disabled except for NUL (0), Ctrl-A (1), and 129. As the tables show, Kermit outperforms the competition every time.

Kermit News Number 5, July 1993 Page 13

Table 2 shows the figures for transferring all four files with each of the four protocols on same direct connection used for Table 1. In this and the following tables, the secs column shows the elapsed time of transfer in seconds, the cps column shows actual file characters transferred per second, and the eff column shows the percent efficiency (file characters per second divided by the connection speed). Table 2 X- Y- and ZMODEM vs Kermit on a 19200-bps Direct Connection

XMODEM YMODEM ZMODEM KERMIT File Type secs cps eff secs cps eff secs cps eff secs cps eff ASCII Text 89 1549 81% 76 1814 95% 73 1889 98% 69 1999 104% UNIX Binary 15 1638 85% 13 1890 98% 13 1890 98% 9 2648 138% PC Binary 127 1558 81% 109 1816 95% 107 1850 96% 100 1979 103% Precompressed 153 1559 81% 133 1794 93% 130 1835 96% 129 1849 96%

Table 3 shows the results for a local-call dialup connection using Telebit T3000 modems, V.32bis modulation (14400 bps), V.42 error correction, V.42bis compression, RTS/CTS hardware flow control, and an interface speed of 57600 bps. The efficiencies in this table are based on the modem’s 14400-bps connection speed, and therefore also reflect the modem’s compression methods. Table 3 X- Y- and ZMODEM vs Kermit with High-Speed Modems

XMODEM YMODEM ZMODEM KERMIT File Type secs cps eff secs cps eff secs cps eff secs cps eff ASCII Text 221 624 43% 79 1746 121% 42 3283 228% 39 3535 246% UNIX Binary 32 768 53% 13 1890 131% 15 1638 114% 3 8192 569% PC Binary 346 572 40% 129 1534 106% 83 2385 166% 80 2474 172% Precompressed 500 477 33% 208 1147 79% 149 1601 111% 148 1612 112%

So far we’ve looked only at connections with no delays. Table 4 (also see cover, left group) shows the results for a V.32 9600-bps cross-country dialup connection from the same PC to a PC/486-50 running UNIX System V R4, with the same C-Kermit, sx, sb, and sz software as on the Sun. The round-trip delay is a fraction of a second. No error correction or compression is done by the modems, but the connection is clean and no errors occurred. Table 4 X- Y- and ZMODEM vs Kermit with Delays at 9600 bps

XMODEM YMODEM ZMODEM KERMIT File Type secs cps eff secs cps eff secs cps eff secs cps eff ASCII Text 422 327 33% 253 545 57% 217 635 66% 151 913 95% UNIX Binary 73 337 35% 41 599 62% 32 768 80% 8 3072 320% PC Binary 536 369 38% 319 620 65% 271 730 76% 207 956 99% Precompressed 710 336 37% 363 657 68% 314 759 79% 284 840 87%

But if we always had clean connections, why would we need error-correcting file-transfer protocols? Table 5 (and middle group, cover) shows the results for the same cross-country connection, same settings, but with short bursts of noise injected every two seconds, which cause errors and retransmissions in all four protocols. Table 5 X- Y- and ZMODEM vs Kermit with Delays and Noise at 9600 bps

XMODEM YMODEM ZMODEM KERMIT File Type secs cps eff secs cps eff secs cps eff secs cps eff ASCII Text 3346 41 4% fail 0 0% 438 315 33% 206 669 70% UNIX Binary 573 43 4% 58 424 44% 144 171 18% 9 2736 284% PC Binary 5154 42 4% fail 0 0% 566 350 36% 281 706 74% Precompressed 5917 40 4% fail 0 0% 694 344 36% 385 621 65%

Page 14 Number 5, July 1993 Kermit News

What about 7-Bit Connections? No Contest!

The foregoing benchmarks were conducted in environments where XMODEM, YMODEM, and ZMODEM can work, namely 8-bit transparent connections that are not sensitive to any control characters. Now let’s look a different, but very common, situation. Table 6 (and right group, cover) shows the results of downloading the same files from an IBM Mainframe running VM/CMS and Kermit-370 4.2.5 to the PS/2 over a 19200-bps serial connection through an IBM 7171 protocol converter, which uses even parity and Xon/Xoff flow control. Kermit’s window size is 1 because the mainframe can operate only in half duplex, and the packet length is 1920, the largest allowed by the 7171. All control characters are prefixed.

Table 6 File Transfer on a 7-Bit Connection

XMODEM YMODEM ZMODEM KERMIT File Type secs cps eff secs cps eff secs cps eff secs cps eff

ASCII Text - 0 0% - 0 0% - 0 0% 81 1702 88% UNIX Binary - 0 0% - 0 0% - 0 0% 9 2730 142% PC Binary - 0 0% - 0 0% - 0 0% 162 1221 63% Precompressed - 0 0% - 0 0% - 0 0% 243 981 51%

The table shows Kermit file transfer to be infinitely more efficient than X-Y-Z-MODEM transfer with IBM mainframes, because X-Y-Z-MODEM implementations do not work with IBM mainframe operating systems such as VM/CMS, MVS/TSO, or CICS, whereas Kermit works with all of them. Of course, 7-bit connections are not peculiar to IBM mainframes. They are also used by other types of mainframes and front ends as well as many types of networks and devices, including some X.25-based public data networks and certain terminal servers. You can use Kermit to transfer files on these connections, but not X-Y-Z-MODEM protocols.

Locking Shifts

Although Kermit, unlike X-Y-Z-MODEM, can transfer 8-bit data over 7-bit connections, there is often a performance penalty. This penalty is particularly unfair to people whose written languages are encoded primarily in 8-bit characters, as are Russian, Hebrew, and Japanese. Russian text encoded in any of the commonly used 8- bit Cyrillic character sets typically consists of about 80% 8-bit characters and Japanese Kanji text often consists of nearly 100% 8-bit characters.

Table 7 shows the results of attempting to upload typical Russian and Japanese 8-bit text files over a 19200-bps 7-bit serial connection to an IBM mainframe using X-Y-Z-MODEM (it can’t be done), Kermit with only single shifts (SS), and Kermit with locking shifts (LS). The Kermit window size is 1 and the packet length is 1920. In these cases, locking shifts improve the speed of transfer 30–40%.

Table 7 Effect of Locking Shifts

X-Y-Z-MODEM KERMIT (SS) KERMIT (LS) File Type Size secs cps eff secs cps eff secs cps eff

Russian Text 52046 - 0 0% 55 946 49% 39 1334 69% Japanese Text 29706 - 0 0% 34 873 45% 20 1485 77%

Conclusion

Kermit protocol works in practically every communication and computing environment. You don’t have to be a data communications expert to transfer a file with Kermit software. Its first priority is getting your data through safe and sound, and its second is efficiency. Kermit’s conservative protocol defaults reflect these priorities: First make it work, then make it fast. But as the tests show, today’s Kermit software, when given several simple commands to enable its efficiency features, outperforms X-, Y-, and ZMODEM protocol transfers every time. And real Kermit software also outperforms the Kermit protocol implementations found in commercial and shareware communications programs. Skeptical? Run your own tests!

Kermit News Number 5, July 1993 Page 15

Kermit and the British Relief Mission to Bosnia

Lieutenant Colonel John F. J. Allen, MBE Royal Logistic Corps, UK Army, Andover, Hampshire, UK

We hear daily of the huge amounts of food and aid brought into the besieged areas of the former Yugoslavia, and we have a successful system, proven in an operational environment, that has now come of age. Further developments will see direct satellite communication to and from relief convoy escort vehicles, and integrated information and communications __ systems and at their heart lies Kermit.

Browsing through our software library last autumn No further visibility was currently available beyond in search of inspiration, I chanced to stumble across this. Future fourth-generation information systems an early version of MS-DOS Kermit that recalled a were also under development, but those components passage I had read on Kermit a couple of years ear- that would link issues to freight consignments to suplier in a communications textbook. I had the germ of port asset tracking were not to be in service in the an idea and, a few trans-Atlantic phone calls later, I immediate future. found myself in New York for my first visit to the United States in late October 1992, about to meet the Our aim was therefore to produce an overarching Kermit team at Columbia University. But to put the mantle system in support of humanitarian missions tale in fuller perspective . . . in Bosnia, based upon a central data repository with information access points across the supply and dis- Once the political decision was taken for British par- tribution chain. The system would address the reticipation in the United Nations relief mission to the quirement of the British contingent on United Naformer Yugoslavia, preparations for deployment tions relief work, presenting visibility of items from began in earnest. For the Army Logistic (G4) area, source to destination. It would achieve the resupply this meant the responsibility for supply and equip- operation as economically as possible and with a ment management support to the United Kingdom more effective, efficient method of control. force deployed in Bosnia. The system presupposed a central distribution point Accountability and total asset visibility of consum- in the Theatre of Operations and the despatch of ables, stores, and spares would be vital to the UN items for the relief operation to the forward areas in mission in the relief areas. The requirement became the former Yugoslavia from single points of departure evident: to establish a system of adequate controls for in the Base or Forward Depots in the United Kingasset tracking and in-transit visibility from point of dom and Germany. despatch in the base area to the receiving distribu- __ tion point in theatre a logistic-support asset- The asset tracking system would require a database tracking system. With such a plethora of commercial using data captured at issuing depots and at various systems available, neither the hardware or software points in the distribution chain. Data on commodity solutions were insurmountable. But selection of com- visibility would then be drawn from the system, munications and file transfer protocols would require through communications links at the source, transit careful consideration. points and destination, with the ability to generate reports and produce meaningful data on location, con- No current computer system specifically addressed tent, quantity and status. storage and distribution commodity tracking, although progress was being made in a number of re- The solution, within the limitations of the time perlated areas that would integrate in later years to mitted, was found by developing an operational provide in-transit visibility of assets. Provision was prototype, followed by a two-phase development, from made within the ICL 3900 Series mainframe-based initial research and development undertaken within Stores System accessed through an online informa- the aegis of a peripheral peacetime project. Project tion system, and other operational and administra- VITAL (Visibility In Transit Asset Logging), was tive information systems, to link demands to issues, therefore highjacked and harnessed to our needs in and track containers in the logistic pipeline. support of the UN operation.

Page 16 Number 5, July 1993 Kermit News

Procedures were put in place to enable information Verification is carried out on-line with Kermit file gathering and to advance and modify relevant transfer and terminal emulation, to the stores system aspects in the prototype development to satisfy the to complete the loop on the status of the commodities. urgent operational requirement. At this stage, after The system is able to operate in either direction. comparison with proprietary commercial software, Kermit was identified as the proper solution to our file The system tracks the progress of commodities, as transfer, network protocol, and terminal emulation single items or as part of larger consignments, along needs, linking the entire spectrum of the project opera- the pipeline, by air, road, rail, or sea routes, and may tion, from mainframe, minicomputer, PCs, to hand- also be applied to postal despatch of items. Items are held devices and barcode readers. identified through a designator code, to combine with transit information, to allow visibility of progression Once the decision was made to proceed, funding was along the pipeline through to the troops deployed on negotiated and development proceeded in two distinct relief convoy work. phases: (1) the basic system that can be put in place quickly, and (2) aspects of the system that would re- The development software to support the immediate quire more investigation and analysis. urgent operational requirement was in service during November 1992, with Phase 1 work complete in PC access points to the system, using IBM-compatible December 1992. Communications links and user soft- 386 SX PCs with printers and necessary software, ware were successfully tested over line and satellite were installed at multiple locations along the supply and the prototype system went live in December and distribution chain to the forward bases that had 1992, with Phase 2 completion due in 1993. Links for been established in Bosnia. air freight are being developed and have been established with the Royal Air Force (RAF) and civil airline air cargo systems.

The profile of the system envisaged a central computerised repository of commodity and transit data, hosted on a UNIX-based ICL DRS 6000 machine, We hear daily of the huge amounts of food and aid drawn from existing logistic information systems, brought into the besieged areas of the former Yugosthis information being accessed and supplemented at lavia, and we have a successful system, proven in an nodal points along the logistic pipeline, and at opera- operational environment, that has now come of age. 2 tional or logistic Command and Control (C ) Head- Further developments will see direct satellite comquarters, using Kermit and data communication links munication to and from relief convoy escort vehicles, to provide the required visibility. and integrated information and communications __ systems and at their heart lies Kermit.

The heart of the system is a relational database, situated at the Directorate of Logistic Information The verdict: We have been most impressed with Ker- Systems, in the county of Oxfordshire, that draws in- mit in all its forms, especially with the support, verformation from the Stores System mainframe, and satility, the ease of use, and lack of problems. We data from the VITAL input devices. were not previously aware of its potential and capabilities, but now we are adapting it in several other systems and extending its use amongst diverse infor- The system is linked on a network by line or Hayesmation areas.

compatible modems through national and international ISDN telephone and through INMARSAT-C satellite communications, through the British Isles A very big thank you to the Kermit team at Columbia commercial communication hub in Cornwall in the University in New York City, who most generously South West of England. Each access point has a PC, cooperated on the project, giving consultancy during a enabling each station to interface to the data whistle-stop visit to New York, including rapid repository through the network. development of prototype scripts for automated connection establishment, authentication, and data transfer, and their continued help desk support and Handheld Tandy-Grid (US model 2350) electronic further software upgrades.

palm-pad data input devices with inductive pen contact and character recognition on touch-sensitive screens, again using MS-DOS Kermit loaded on SUN The author, Lieutenant Colonel John F. J. Allen, RAM disks, are in use along the logistic pipeline, al- MBE, is a career officer in the UK Army in the newly lowing electronic download of data through the PCs, formed Royal Logistic Corps, responsible for Logistic or direct over the communications links, to the Support Information Systems Policy and Strategy curcentral database, and data retrieval, screen and rently serving at the Ministry of Defence Logistic report printing at each access point. Headquarters in the South of England.

Kermit News Number 5, July 1993 Page 17

Sounds familiar? Yes, there we are: Kermit fits the

Kermit in Germany_{bill nicely. So, somewhat unexpectedly, we have a}

whole new market for Kermit software. And this ex- Gisbert W. Selke tends to other parts of Eastern Europe as well: since Ermekeilstra_e 28 I’m giving a hand with Kermit promulgation on this D-5300 Bonn 1, Germany side of the Atlantic, I have noticed a considerable demand for Kermit software from Poland, Czechoslo- Over the past several years, three major events have vakia, and even as far as Kazakhstan, when it still happened to Germany: was a part of the Soviet Union.

• Re-unification of East and West, Kermit and German Text • the advent of umlaut-preserving file transfer, For decades, computers have been made by English- • and a German MS-DOS Kermit book. speaking people for English-speaking people. But German, like many other languages, has special char- While there is no direct causal connection between acters that do not fit into standard 7-bit ASCII code any two of these, they are not altogether unrelated (which, after all, is the American Standard Code for either; so let’s look at each of them in turn. Information Interchange).

First, re-unification. After nearly 50 years, the Iron So, various manufacturers have looked for ways to Curtain that separated the Western 75% of the_{__} circumvent this. One way of doing this with the population from the Eastern 25% has at last been_{__} ISO’s blessings was to scrap the braces, brackets taken down. Everyone will have read in the papers and so forth and use their character positions for the about this, so we won’t go into the details here; just umlaute. This was widely accepted; but what if you let me say that it feels great to be able to see my needed those braces?

relatives dryben (over there) whenever I want.

Your beautiful C programme, when printed on a ger- Apart from my personal feelings, however, there is manicized printer, might look like this:

one aspect that has, in fact, to do with computing and, more specifically, with Kermit: the computer if ((a==1) ss (a==9)) c market, both private and business, is a hot spot in printf("Gry_e aus KslnSn");

y

the region commonly referred to as the ‘‘5 neue Lcnder’’ (or 5NL, for short, although Americans However, if you switched the printer back to plain might prefer the colloquial ‘‘Neufynfland’’). ASCII, your programme would look like this:

if ((a==1) || (a==9)) {

And so is the telecommunications market. While printf("Gr}~e aus K|ln\n"); telephones have been hard to come by previously, the } German PTT is bustling to bring the telephone net up to standard, for which there is an enormous need. Not what you intended, either . . . And no way around it. With the advent of the IBM-compatible Together, these factors have created high demand for PC, a different standard emerged, which at least computer communications. The 5NL universities preserved normal ASCII as well as many European have joined the Internet, and private mailboxes special characters. The Macintosh, of course, was dif- (BBS’s) are mushrooming. For many purposes, ferent. And of late, Windows has yet another conceptelefax is the service used heavily between the two tion of the special characters. You are not, of course, parts of Germany, but there are also many companies surprised to hear that MS-Windows NT is almost enthat have to exchange data between their Western tirely unlike the others. head offices and their Eastern branches (note the asymmetry here!). As time went by, we gained some proficiency in deciphering on the fly. Depending on the machine Since currently the Eastern phone net is still in you’d work with, you’d know what key (or sequence of deplorable shape in many places, a reliable, yet fast keys) to type to get the desired letter. What, file transfer protocol is needed. Of course, it should however, if you had to exchange files between difbe easily adjustable to take advantage of improving ferent platforms? Let me recall one early day in the conditions; it should be able to handle those funny WIdO (Wissenschaftliches Institut der Ortskrankencharacters (like c and _) that Germans seem to like kassen), where we had been running a Modcomp so much; and implementations should be easy to MAX IV as a host computer for years, and the first handle, since you wouldn’t want to employ a com- PCs arrived and were wired up as terminals over the puter scientist just for this purpose. serial line. Boy, were we happy to have found MS-

Page 18 Number 5, July 1993 Kermit News

DOS Kermit 2.28 to transfer files in the first place! Kermit auf Deutsch

But then we sent an ordinary (or so it seemed) text_{__} Well, there we are, with Kermit a programme to cater file from a PC to the host. For the greater part, all to all the Germans’ communication needs. There was went well; but some characters were missing, and only one problem remaining: the only Kermit strange runs of repeated characters could be found in documentation available was in English. Not too places. much of an obstacle for your local hacker . . . But it’s

sometimes good to remember that there are ordinary The explanation turned out to be simple: characters people, too, to whom a computer and a modem are with their eighth bit set were a special MAX code just tools and who don’t want to have to learn a used for a simple run-length encoding. Annoying, foreign language just to use these tools. (Conversely, yes; and although it was easy to write a programme it is sometimes worth noting that there are people to convert the umlaute to braces and brackets, who can actually type and not just chase a rodent Murphy’s Law tells us that you would forget to use around on their desktop. But I digress.)

this filter on none but the largest files . . .

Fortunately, Chris Gianone had written an excellent Today, all this is gone. Using MS-DOS Kermit, I can book on MS-DOS Kermit; not just a manual, but a easily configure my ‘‘terminal’’ to display braces as gentle introduction into terminal emulation and file umlaute: SET TERM CHAR GERMAN! Or, to show them transfer. While she was taking this book to its as braces, SET TERM CHAR LATIN1, as would be used second edition, covering all the new features since with a host employing an ISO 8859-1 character set MS-DOS Kermit 3.0, she was looking for foreign- (which, incidentally, is also used by MS-Windows)._{__} language publishers as well. And we made it a Our secretaries no longer have to remember to hit ’[’ publisher known for high-quality magazines and __ when they want ’C’ to be printed some progress! books on all aspects of computers and electronics Or, when I connect to an IBM VM/CMS mainframe proved to be interested, indeed. Nearly in parallel to (an EBCDIC machine), accidentally hitting one of the Chris’s writing the second edition, I prepared the umlaute on my PC keyboard tended to wreak havoc German translation, so the German book appeared on on the connection. Nowadays, I have a few comthe market barely three weeks later than the Amermands like: ican original. The representative of the American

SET KEY C Ae publisher couldn’t quite conceal his astonishment

in a special TAKE file, and whenever I hit the C key, when presented with the German translation at the

‘‘Ae’’ is sent instead (where Ae is the standard trans- October 1991 Frankfurt Book Fair, and our German_{__}

literation for C, from auld lang pre-computer syne). editor took some pride in this rightly so! By the

way, all the queries and last-minute corrections be-

File transfer, too, is no longer a problem. On our tween Chris and myself were done using Kermit soft-

UNIX host, we use C-Kermit; sending a file to the ware (making Kermit a recursive application?).

MAX host, we can SET FILE CHAR LATIN1, SET TRANS-_{__}

FER CHAR ASCII, and SET LANGUAGE GERMAN, and all At 69 marks, MS-DOS-Kermit das universelle Kom-

the umlaute are converted automatically to braces, munikationsprogramm includes the official Kermit

etc., on the fly. As I write this, the old MAX IV host distribution disk with all the text files translated into

is being taken down and replaced by a MAX 32; and German. To my knowledge, this is the first book on

here’s another advantage for us: no more serial links the German market to cover computer communica-

at 9600 or 19200 bits per second, for now we’ve got an tions at this scope, and the sales figures show that it

Ethernet! And, surprise, Kermit supports LANs, too; fills a need: it is selling well, so get your copy before __ no need to change to any other Telnet terminal emu- they are sold out! OK, don’t panic... the second

lation programme, no need to give up Kermit’s speed, printing has just hit town. (Which shows that the

easy configurability and robustness. book is more successful than had been anticipated by

the publishers themselves.)

There was even a story about a user who wanted to

convert a German text file from PC standard to the Hold the presses! Here we go again: Frank da Cruz

newer Windows standard. So he started Windows, and Chris Gianone have collaborated on a mag-

ran MS-DOS Kermit in two different windows, nificent book on C-Kermit. C-Kermit runs on an

hooked up COM1 and COM2 with a null-modem amazing variety of machines whose least common

cable, SET this, SET that, and off he went, com- denominator is just the existence of a C compiler. It’s

municating with himself, so to speak, but trans- a natural for all those UNIX machines, of course; but

literating the file in the process. This story was re- it also runs on . . . no, wait, I’m not going to bore you

lated at a Rhineland Karnival session, so take it for with a list several pages long. Why not browse your

what it’s worth . . . friendly local book-seller’s shelves? You say you’re

Kermit News Number 5, July 1993 Page 19

living in Austria (the one without kangaroos) and you Fortunately, we found the article written by Frank da don’t exactly fancy manuals in English? No problem: Cruz and Bill Catchings in BYTE magzine and realthe German translation is underway right now, and ized that Kermit was just what we were looking for! you’ll be able to pick it up at the Frankfurt Book Fair After receiving tapes containing all Kermit programs in early October. And, lest I forget: if, by ‘‘manual’’, and documents from Columbia University, we wrote you mean ‘‘dreary and unreadable,’’ you’re dead I/O driver routines for the Data/Voice integrated comwrong. Were it otherwise, I wouldn’t have translated munication adapter, a powerful network card used in it. I can’t stand boring books. ZUnet that handles data and voice simultaneously. Then we modified MS-DOS Kermit 2.32/A and C- Kermit 4E to make them run on ZUnet. Because CC- Let me mention a final point that is often overlooked. DOS (the Chinese version of DOS used in IBM-PC Kermit software has the greatest user support I have and its compatibles) is widely used in ZUnet, we also ever seen. This shows in fast response to (even modified MS-DOS Kermit 2.32/A for Chinese DOS minor) complaints, in lots of care spent on the fine and named it CC-Kermit 2.32/A [On Tape C].

points, and, of course, in the concern given to the nonstandard user. Among these, I count the non-English speakers, but also those with visual, auditory or Kermit and Chinese DOS physical challenges. This concern does not go without saying in today’s computer market; and, speaking for In China, the most popular microcomputers are IBM the non-English people at least, I’d like to say thanks PCs and compatibles. CC-DOS (or CDOS) is a Chito Frank da Cruz (who started it all, and who spends nese DOS for PCs, which has many different vera lot of time on C-Kermit), to Chris Gianone (who sions; basically it is MS-DOS with Chinese character keeps it all running and whose book is terrific) and to I/O processing modules. Most application manage- Joe Doupnik, whose programming skills I won’t even ment systems run under CC-DOS. From the user’s mention, but whose wit and understanding have point of view, characters are displayed on the screen proven invaluable over all those years since I first got in character mode, but from the system’s point of in touch with MS-DOS Kermit version 2.28. view, Chinese characters are actually displayed in graphic mode. In general, a Chinese character code is represented by two bytes. The IBM PC version of MS-DOS Kermit can’t run correctly on CC-DOS be-

Kermit in China_{cause it accesses video RAM directly.}

Quanfang Zhang and Jijiao Zheng We converted MS-DOS Kermit 2.32/A to CC-Kermit Department of Computer Science and Engineering 2.32/A, a Chinese Kermit, which can run on MS-DOS Zhejiang University, Hangzhou, China and most versions of CC-DOS. Explanations and

prompt messages are displayed in Chinese when it Today, Kermit has spread all over the world and has runs on CC-DOS. This is very important for the been implemented in many computer systems. popularization of Kermit in China, as many users do Quietly, it arrived in China and was adapted to many not learn much English. When it runs on MS-DOS, Chinese-version operating systems. You can see CC-Kermit is the same as MS-DOS Kermit 2.32/A. more and more computer specialists and users using Kermit to transfer files or connect a local computer to Chinese character codes are defined by Chinese Chara remote host in Chinese universities or institutes. acter Set for Communication and its Exchange Codes, Kermit is now a popular topic for discussion among GB2312-80. The size or resolution of a Chinese charpeople who are engaged in computer communications. acter displayed on the screen can vary. There are

16× 16, 24× 24, 32× 32 and 48× 48 dot matrices, As teachers in the Department of Computer Science depending on the CC-DOS and graphic adapter verand Engineering of Zhejiang University, we are very sions. We modified the display and keyboard input interested in computer networks and communica- modes of Kermit for various display sizes, such as 11, tions. We began to study Kermit at the end of 1988, 17, or 25 lines per screen. when our Computer Network Research Laboratory was entrusted with designing the Zhejiang Univer- Kermit at Zhejiang University sity campus computer network (ZUnet). In the first stage of development, we planned a network system At Zhejiang University, there are more than 1000 based on a PBX. We found it very difficult to design computers including microcomputers (IBM PC, Apple such a network because many computers, distributed II/III, etc.), minicomputers (MicroVAX II/III, VAX in all departments and administrative offices and 11/785, PDP-11/23) and two mainframes in the Comrunning many different operating systems, would be puting Center (Honeywell DPS8 and IBM 4361).

connected by ZUnet. There are also a lot of HP and Sun graphics worksta-

Page 20 Number 5, July 1993 Kermit News

tions. Teachers and students used to find file transfer Report from London: between two machines annoying. Now Kermit makes Kermit in Medical Research it simple.

Robert Clark Kermit plays an important role in ZUnet. There are Joint Computing Unit, Institute of Neurology, over 60 computers in ZUnet distributed in 12 build- University of London, Queen Square, London ings. ZUnet makes use of the existing telephone system; each computer is equipped a Data and Voice in- The Institute of Neurology is a postgraduate medical tegrated adapter with data transfer at speeds up to research Institute of the University of London, closely 19200 bps. ZUnet is a low-cost but useful system. It linked with the National Hospital for Neurology and provides file transfer, eletronic mail, database re- Neurosurgery and an internationally renowned centrieval, terminal emulation, and remote job entry. tre for teaching and research in neurology and the neurosciences. The Institute of Child Health is Users can exchange e-mail internally and with CAnet responsible for research and teaching within the field (China Academic Network), and we are connected by of child health and p3diatric sub-specialities, and is Kermit to a host in Beijing for international electron- closely associated with the Hospital for Sick Children ic mail. Computer specialists consider ZUnet an eco- at Great Ormond Street. Since the two institutes are nomical, useful, and efficient campus network, well- next door, a Joint Computing Unit was formed to look suited to universities and institutes of China. after the information technology needs of academics, medical researchers, clinicians, scientists, adminis- Kermit in China trative and library staff. It is in this heterogeneous environment that Kermit has proved to be a most Kermit is widely used not only at Zhejiang University versatile and valuable tool. but also in many other places in China. Users scattered in different districts in Zhejiang Province use Initially the predominant use of Kermit was for main- Kermit to connect to the host at the Scientific and frame access via Packet/Assembler/Disassemblers Technological Information Institute of Zhejiang (PADs) linked to Britain’s X25 Joint Academic __ Province to retrieve databases. In ShengLi Oil Field, Network JANET. Kermit was also used extensively the second largest in China, a whole oil-field infor- for micro-micro file transfers. In the days of CP/M, mation management network system is being built. every machine seemed to differ with respect to disk The system is composed of a lot of computers dis- format, and Kermit liberated data. Even when Kertributed in the Oil Field headquarters, oil extraction mit did not exist for particularly idiosyncratic factories, oil production teams, and well drilling machines, we still could use it for data transfers. teams. Kermit protocol and software are used in the large systems.

Perhaps the most interesting and topical use of Kermit is the way its elegant

Papers about Kermit have been published in many

terminal emulators are being used in

Chinese computer magazines. including an article by us, Kermit Protocol and its Programs, presenting the AIDS research. background, development, running environment, functions, and protocol of Kermit, published in Chinese Data Communications, No.2, 1991. For example, we had to replace several dozen harddisk Z80 machines with a multiuser operating system Kermit has already played an important part in (TurboDOS) for which there was no Kermit [There is China, especially in Zhejiang University. We are now! –Ed.]. Fortunately TurboDOS had a hex dump sure that it will be recognized by more and more com- and a CP/M batch capability. We replaced dumb terputer users and become their good friend. Kermit minals connected to TurboDOS machines with PS/2s makes complicated things simpler and longer dis- running Kermit._{LOG SESSION} was used to capture tances shorter. We hope to make and keep contact directory listings from the TurboDOS machine which with other Kermit developers and work together for were then processed to produce a BAT file with a the development and populization of Kermit. series of dump commands. This was_{TRANSMIT}ted to the TurboDOS machines into a WordStar document We would like to express our sincere thanks to Chris- and saved. The BAT file was then executed and_{LOG} tine M. Gianone and Frank da Cruz for their pro-_{SESSION} was used to capture the hex dumps. A small tracted support and guidance to us. Without their BASIC program converted the hex back to binary. In help, our ZUnet could not have been put into working this way several years and megabytes of medical text order in such a short time. and data were rescued from oblivion.

Kermit News Number 5, July 1993 Page 21

Another useful role of Kermit has been in the area of data capture. Many of the departments have medical data acquisition apparatus that produce ASCII data on a serial line. Establishing the appropriate communications parameters (baud rate, number of bits, parity, etc.) is easy with Kermit, as you can make changes until you see what looks sensible on the screen. Having established parameters, Kermit then becomes a production tool, using LOG SESSION to capture data for subsequent analysis. Typical of this is our Neuropathology Department who use a light pen with digitising apparatus to trace around the inner and outer circumferences of cross-sections of cells photographed on an electron microscope. The aim of this is to determine the thickness of the cell walls, as with the progression of neurological disease, cell walls get thinner. An analysis of the distribution of the thicknesses of cell walls from a representative Figure 1 Age vs CD4 Count sample gives a prognostic indication. Kermit captures the data with LOG SESSION for subsequent diagnosing HIV infection is of no value for infants. analysis by statistical packages. As HIV infection causes a lowering of CD4 cell count, p3diatricians attempt to monitor changes in CD4 On a more general level, Health and Safety Regula- levels to identify infected infants. But satisfactory tions require all departments to check laboratory ap- ‘‘normal’’ age-related curves for CD4 count do not exparatus for electrical safety on an annual basis. The ist for children. checking apparatus is attached to a Toshiba portable; data is captured by Kermit for subsequent print-out At birth, CD4 count is relatively high; it rises further back at base. to peak at about 6 months before tailing off slowly to adult levels. The department is currently developing In addition to research and laboratory work we use age-related standards for CD4 counts using blood

__ __

another feature of Kermit the script capabilities for samples taken from children from the study who were administrative purposes. We have a number of X.25 subsequently found to be uninfected. To create the PADS and two X.25 switches that need detailed and curves the data is analyzed by being ‘‘chopped’’ into longwinded configurations. The configuration on intervals and deskewed within each interval. This these devices is held in battery-backed RAM on a transformed data is then plotted in Tektronix emulaloader board. From time to time these boards fail and tion and curves are fitted. over one hundred lines of configuration parameters must be reentered. The configurations are now kept How does Kermit help? Developing the curves beas Kermit scripts which reduce reconfiguration from comes an interactive, iterative modelling process. A a couple of hours to a couple of minutes. In a similar program has been written that allows suitable interway, a Kermit script running on a PC plugged in to a vals to be chosen and entered into a VT320 screen, VAX as a console allows us to automate ‘‘standalone standard deviations are calculated and plotted by togbackups.’’ Manually typing in standalone backup gling the screen into Tektronix mode; if the curve is of commands was a time-consuming and potentially interest it is saved for hard-copy laser printing, the dangerous operation as the VMS DCL procedural lan- screen is then toggled back to VT320 for the next set guage is not available in standalone mode. of intervals to be entered. An example of such a curve is shown in Figure 1. The X-axis shows age in days and the Y-axis shows the CD4 count. Each

Kermit and AIDS Research

curve is a centile at the 3%, 5%, 25%, 50%, 75%, 95% Perhaps the most interesting and topical use of Ker- and 97% intervals, reading from bottom to top. Thus mit is the way its elegant terminal emulators are be- 50% of non-infected children should have a CD4 ing used in AIDS research. The Department of count of about 3.2 at age 200 days. Epidemiology and Biostatistics at the Institute of Child Health coordinates the European Collaborative These curves were recently presented at a workshop Study on AIDS research, a prospective study of on Measurement and Use of CD4 and Other Lymchildren born to HIV-positive mothers in 10 Europephocyte and Immunophenotypic markers in Pediatric an centres. Because maternal antibodies cross the HIV Infection, organised by the National Institutes of placenta during pregnancy, the standard test for Health in Washington DC (October 1992).

Page 22 Number 5, July 1993 Kermit News

My fundamental approach to software selection is to

And Now, TCP/IP

find the most cost-effective solution to our applica- What of the future? Until very recently, like most tions needs. If there exists free software that will do British academic sites, we were entirely X.25-based. the job, we use it. If not, we look at shareware. If Our Joint Computer Unit is part of a consortium of only a commercial package will do, we’ll write the academic computing facilities, the Bloomsbury Com- company and ask that the package be donated. If all puting Consortium. The farsighted directors of this else fails, we’ll buy it. consortium have designed and implemented an architecture based on networked UNIX machines, with a metropolitan area network using TCP/IP protocols. So far, I haven’t found anything that At grassroots level we have had to learn a whole new Kermit can’t do or be taught to do. set of software tools.

Although being part of the Internet is, to say the One application of great importance to us is telecomleast, exhilarating, we found products such as PC- munications. One of our functions is to provide NFS difficult to configure and the TELNET terminal resources and information to health care profesemulators rather limited. The recent TCP additions sionals and the public. So it’s crucial that we are on to Kermit and the sheer readability of the parameters top of what’s going on in the areas of grief, loss, death in an MSKERMIT.INI file has moved us from a situa- and dying specifically and the mental health care tion of struggle to a situation of load and go, whereby field in general. we can bring new connections on stream in a matter of minutes. Finally, we have adapted the excellent Software selection, in this case, was easy. We chose dial-up script supplied with Kermit 3.11 to set PC e- Kermit! With Kermit we can connect to the many mail lists that interface through the e-mail capability different online resources available, find others in our of C-Kermit on various UNIX hosts. It looks as field, and exchange information with them. though we will be using Kermit well into the next millennium. Although there are shareware and commercial pack-

ages which can (probably) do the same thing, for us, Grateful acknowledgement to Angie Wade and David Kermit is the logical choice for the following reasons: Dunn, Department of Epidemiology and Biostatistics, 1. Kermit is inexpensive both in terms of cost and hard- Institute of Child Health, University of London and to ware resources.

Peter Sacares, Statistician, Institute of Neurology, University of London. 2. Kermit is what Esperanto was supposed to be. Everyone speaks it. This is really important as we connect to a variety of systems including Library Bibliographies, File Servers, Bulletin Board Systems,

Kermit in a Nonprofit Environment_{and Commercial Databases. In other words, at any}

one time we may connect to a micro, mini, or main- Buz Overbeck, President frame computer where Kermit is the only common Grief Resource Foundation, Dallas, Texas, USA denominator.

3. Kermit is now ‘‘Competitive’’. When I first used Ker- Selecting software for a new nonprofit organization mit, I had trouble adapting it to the micro world of can be very challenging! Unlike most large corpora- BBS systems due to the lack of documentation in this tions, whose budget allows the purchase and/or eval- area. For that reason, I almost passed on Kermit for uation of large expensive packages, nonprofits, unless the Foundation. But then came Using MS-DOS extremely well funded (a rarity), seldom have the Kermit by Christine M. Gianone. That changed money to buy many large packages, nor the name everything. Here, in one place, was the answer to almost every concern I had. No more excuses.

recognition to receive evaluation copies from vendors.

So, we adopted Kermit. This decision allowed us to The Grief Resource Foundation falls into this cateput the money budgeted for an expensive communigory. Our funding comes from the sale of our publicacations package to better use. Since then, we’ve betions and services, grants, and donations. The fundcome pretty Kermit-literate. So far, I haven’t found ing we receive is plowed back into the research and anything that Kermit can’t do or be taught to do.

development of new services, with little left over for software. Like many nonprofits, we pay all of our And for telecommunications at the Grief Resource bills on receipt which means we have no credit his- Foundation, Kermit is the package of choice. I only tory. This alone disqualifies us from a corporate acwish that other application solutions were as obvious.

count at, say, Egghead Software, which would be very useful to us.

Kermit News Number 5, July 1993 Page 23

Miscellany

dress and interrupt of any serial device, COM1

Modem Watch

through COM4, and it treats the device with special Around mid-1992, the market was inundated with care so as not to tickle the many bugs that have surlow-cost, high-speed V-Dot-Everything modems and faced in these products. 14,400-bit-per-second communication was suddenly as affordable as 2,400 bps was just a few years ago.

Acknowledgements

The TIES That Bind Because of space constraints in this issue of Kermit News, many acknowledgements were omitted from One of the factors that contributes to the low cost of their proper places. Kermit software development is these newer modems is their elimination of the esa worldwide voluntary effort on the part of thousands cape-sequence ‘‘guard time.’’ The guard time of programmers, testers, and ordinary users who prevents accidental return to the modem’s command report problems or make suggestions. You already processor when the data stream happens to contain know the magnificent work of Joe Doupnik and John the escape sequence (most commonly +++). If the +++ Chandler. Special thanks to Mike Normile of Data is not preceded and followed by a full second of in- General Corporation for supporting and assisting activity, it is transmitted safely rather than triggerwith major portions of MS-DOS Kermit 3.13 developing an unwanted escape. The guard time concept is ment, and also to Novell (and particularly Brian patented by Hayes Microcomputer Products, Inc. To Meek), to Microsoft, Inc., to Beame and Whiteside, cut costs, some modem manufacturers no longer sup- Inc., and to Interconnections, Inc., for additional corport guard time. These companies say they have porate assistance, and to Moshe Solow and Shalom adopted a new ‘‘technology,’’ which they call Time-In- Mitz at Hebrew University, Gudmundur Bjarni dependent Escape Sequence, or TIES, in its place. To Josepsson at the University of Iceland, Hirofumi Fujii reduce the risk of accidental escape, some (not all) of the Japan National Laboratory for High Energy TIES modems require the escape sequence to be fol- Physics, and to James Sturdevant and John Chandler lowed by a valid modem command, for example: for important information, code, and/or testing of new

+++ATH0

features. To illustrate the effects of TIES, suppose the modem’s C-Kermit 5A, written by Frank da Cruz of Columbia escape sequence was +++ and you wanted to upload University, is the result of a massive three-year effort this article through a TIES modem, using ASCII, that also involved countless experts in UNIX, VMS, XMODEM, YMODEM, ZMODEM, UUCP, or most OS/2, AOS/VS, and other operating systems and their other protocols. As soon as ‘‘+++ATH0’’ arrives at the legion variants and releases. The list of contributors modem, the connection hangs up. to its development takes up five pages in Using C-Kermit! To list only a few:

The good news: It won’t happen during a Kermit_{Chris Adie (Edinburgh U, Scotland), William Bader (Software Consult-} file transfer. All the popular Kermit software ver-_{ing Services, Nazareth, PA), Fernando Cabral (Padrfo IX, Brasllia,} sions, including the current releases of MS-DOS Ker-_{Brazil); Joe R. Doupnik (Utah State U); Stefaan Eeckels (Statistical} mit, C-Kermit, Mac Kermit, and IBM Mainframe_{Office of the European Community, CEC, Luxembourg); Kristoffer} Kermit are TIES-resistent. (Or should we say,_{Eriksson (Peridot Konsult AB, Srebro, Sweden); Marcello Frutig} TIES-compliant?) (Catholic U, Sfo Pfulo, Brazil); Hirofumi Fujii (Japan National

Laboratory for High Energy Physics, Tokyo); William Glass; Andy Fyfe (Caltech); Eugenia Harris (Data General); Charles Hedrick (Rutgers U);

Internal PC Modems_{Christian Hemsing (Rheinisch-Westfclisch Technische Hochschule, Aa-}

Many PC users are attracted by the even lower cost of_{chen, Germany); Terry Kennedy (St Peter’s College, Jersey City, NJ);} internal versions of the new modems, which is ach- Lawrence Kirby (Wiltshire, UK); John Klensin (MIT); Tom Kloos (Se-

quent Computer Systems, Inc.); Bo Kullmar (ABC-Klubben, Stockholm,

ieved by eliminating the case, lights, and power_{Sweden); David MacKenzie (Environmental Defense Fund, U of} supply. The internal modem must be installed in_{Maryland); Fulvio Marino (Olivetti, Ivrea, Italy); Peter Mauzey (AT&T);} your PC in way that does not conflict with existing_{Bruce J. Moore; Paul Placeway; Kai Uwe Rommel (Technische} serial ports or other devices, often as COM3 or COM4_{Universitct Mynchen, Germany); Jay S. Rouman (U of Michigan);} devices, using various interrupts, which tends to_{Fri}rik Skulason (U of Iceland, Reykjavik); Lee Tibbert (DEC); Warren} cause problems with many of our PC communication Tucker (Tridom Corp, Mountain Park, GA); Konstantin Vinogradov

(ICSTI, Moscow, Russia); Eduard Vopicka (Prague School of Economics,

packages, including (until now) MS-DOS Kermit._{Czechoslovakia); Stephen Walton (California State U at Northridge);} Version 3.13 has been adapted to high-speed internal_{Jamie Watson (Adasoft, Switzerland); Rick Watson (U of Texas); Patrick} modems by allowing you to specify the hardware ad-_{Wolfe (Kuck & Associates, Inc.).}

Page 24 Number 5, July 1993 Kermit News

Ordering Information

Kermit software is distributed by Columbia University on magnetic tape, tape cartridges, and certain diskette formats. Tapes and cartridges include all source code and supporting files in machine-readable form for each Kermit implementation, and in some cases also binaries (encoded in hex or other printable format). Diskettes have no source code except when noted on the order form.

Kermit software programs are collected on six reel-to-reel 9-track tapes: A, B, C, D, E, and F. The programs are assigned to tapes A–F as shown in the second column of the Kermit version list as follows: Tape A has the MS- DOS, CP/M-80, and Apple II versions. Tape B has the IBM mainframe and DEC PDP-11 versions. Tape F has C-Kermit. Tape C has other miscellaneous microcomputer, PC, and workstation versions. Tape D has other miscellaneous minicomputer and mainframe versions. Tape E contains machine-readable copies of the Kermit protocol manual, various other manuals, articles, the Info-Kermit Digest, newsletters, a character-set-aware text-to-PostScript printing utility, and tape utilities. Tapes and cartridges are available in these formats:

ANSI: ANSI labeled ASCII, format D (variable length records), blocksize 8192. 9-track, half-inch, reel-to-reel, 1600 bpi. Readable by many computer systems, including VAX/VMS.

TAR: UNIX TAR format, blocksize 10240, 9-track, 1600 bpi. OS: IBM OS standard labeled EBCDIC, format VB (variable length records), blocksize 8192, 9-track, 1600 bpi, for MVS, CMS, and other mainframe systems. IBM VM/CMS users should order the OS format and use one of the included tape-reading programs to read the tape on a CMS system; printed instructions are included with the OS tape.

TK50: TK50 tape cartridge for the DEC MicroVAX or VAXstation. VMS BACKUP format. Also readable by TZ30, TK70, and compatible drives.

QIC: UNIX TAR-format quarter-inch tape cartridge. Readable on Sun computers, IBM RS/6000, SCO systems, and other UNIX systems equipped with QIC cartridge drives.

8MM: EXABYTE 8-millimeter cassette, UNIX TAR format.

Diskettes formats are 5.25-inch 360K and 3.5-inch 720K.

NEWS AND UPDATES

Kermit News is mailed periodically free of charge to all our Kermit customers to bring news of Kermit software releases and related developments. Ordering any Kermit material from us automatically adds you to the subscriber list. We do not have the resources to send automatic software updates. Use the order form on page 27 to obtain new versions of the Kermit software, or call +1 212 854-3703 for inquiries.

TERMS AND CONDITIONS

__ __

The Kermit software including source code is furnished without warranty of any kind, and neither Columbia University, nor the individual authors or publishers, nor any institution that has contributed Kermit material, acknowledge any liability for any claims arising from the use of Kermit. Since source code is available, users may fix bugs and make improvements, and are encouraged to contribute their work back to Columbia for further distribution.

Kermit software may be ordered by private individuals, corporations, academic or government institutions, and other organizations for their own internal use, but the software may not be resold or otherwise redistributed to external clients, customers, or contractors without written permission of the Manager of Kermit Development and Distribution at Columbia University. Contact us for further information.

TO ORDER FROM COLUMBIA UNIVERSITY, fill out and return the enclosed order form. PREPAYMENT by credit card or check is encouraged; an additional ORDER PROCESSING FEE is required if we must issue an invoice. Orders are shipped by delivery service or US mail, normally within 2–4 weeks of receipt, but firm delivery schedules or methods cannot be guaranteed. Prices are in US dollars and include shipping costs. When two prices are shown (like $100 / $135), the first price applies to the USA, Canada, and Mexico and the second price is for shipments to other countries (exception: if you can supply with your Federal Express account number, then pay the first price). Rush service is available for an extra fee. Call +1 212 854-3703 for additional ordering information. Telephone and Fax orders are accepted if payment is by Master Card or Visa. Use the order form for Fax orders, and, for payment by credit card, be sure to include your signature.

Kermit News Number 5, July 1993 Page 25

Operating Program Program Released Operating Program Program Released Prefix Tape Machine System Language Version yy/mm/dd Prefix Tape Machine System Language Version yy/mm/dd

CK F various 4.1-3 BSD C 5A189 93/06/30 K11 B DEC PDP-11 RSTS/E Macro-11 3.60 89/06/13 CK F various 4.4 BSD/A C 5A189 93/06/30 K11 B DEC PDP-11 RSX-11/M,+ Macro-11 3.60 89/06/13 CK F various POSIX C 5A189 93/06/30 K11 B DEC PDP-11 RT-11 Macro-11 3.60 89/06/13 CK F various QNX 4.1 C 5A189 93/06/30 K11 B DEC PDP-11 TSX+ Macro-11 3.60 89/06/13 CK F various UNIX SIII C 5A189 93/06/30 K12 D DEC PDP-12 OS/12 PAL-8 10g 90/09/13 CK F various UNIX SVR2 C 5A189 93/06/30 K11 B DEC Pro-3xx P/OS Macro-11 3.60 89/06/13 CK F various UNIX SVR3 C 5A189 93/06/30 K11 B DEC Pro-3xx Pro/RT Macro-11 3.60 89/06/13 CK F various UNIX SVR4 C 5A189 93/06/30 C86 C DEC Rainbow CPM86 ASM86 2.9 84/12/03 TRI C various TRIPOS BCPL - 87/07/10 MS A DEC Rainbow MS-DOS MASM 3.10 91/03/18 TD C various TurboDOS ASM - 92/10/29 QNX C DEC Rainbow QNX 1.x C 1.0 85/09/23 FLX C various 6809 Flex 9 6809 Asm - 86/04/17 CK F DEC VAX 4.xBSD C 5A189 93/06/30 UF C various 6809 UniFLEX C 1.4 89/02/02 CK F DEC VAX (Open)VMS C 5A189 93/06/30 OS9 C various 6809 OS-9 C 1.5 85/09/20 CK F DEC VAX ULTRIX C 5A189 93/06/30 CK F various 68000 OS-9 C 5A189 93/06/30 CK F DEC VAX UNIX SVR3 C 5A189 93/06/30 OS9 C various 68000 OS-9 C 1.5 85/09/20 VMS B DEC VAX VMS Bliss,Macro 33128 91/01/04 CP A various 808x CPM80 2.2 LASM 4.11 91/04/23 MS A DEC VAXmate MS-DOS MASM, C 3.13 93/07/08 CP A various 808x CPM80 3.0 LASM 4.11 91/04/23 CK F DEC VAXstation (Open)VMS C 5A189 93/06/30 MS A various 80x86 MS-DOS MASM 3.13 93/07/08 CK F DEC VAXstation ULTRIX C 5A189 93/06/30 CP A Access Matrix CPM80 2.2 LASM 4.11 91/04/23 CP A DEC VT-180 Robin CPM80 2.2 LASM 4.11 91/04/23 BBC C Acorn BBC B OS1.20 6502 Assem. 1.45 87/05/19 K12 D DEC VT-78 OS/8 Fam. PAL-8 10g 90/09/13 BBC C Acorn BBC B+,128 OS 2 6502 Assem. 1.45 87/05/19 K12 D DEC VT-278 OS/78 V4 PAL-8 10g 90/09/13 CP A Acorn BBC CPM80 2.2 LASM 4.11 91/04/23 K12 D DECmate I OS/78 V4 PAL-8 10g 90/09/13 BBC C Acorn Compact OS 3 6502 Assem. 1.45 87/05/19 K12 D DECmate II,III OS/278 V2 PAL-8 10g 90/09/13 BBC C Acorn Compact Panos C 4C 57 87/07/14 CP A DECmate-II,III CPM80 2.2 LASM 4.11 91/04/23 BBC C Acorn Master 128 OS 3 6502 Assem. 1.45 87/05/19 MS A DECmate-II,III MS-DOS MASM 2.29 86/05/28 AC C Acorn Workstation PANOS C - 87/07/13 CK F DECstation OSF/1 C 5A189 93/06/30 MS A ACT Apricot MS-DOS MASM 2.30 88/05/12 CK F DECstation ULTRIX C 5A189 93/06/30 CP A Action Discovery CPM80 2.2 LASM 4.11 91/04/23 K10 D DECsystem-10 TOPS-10 Bliss, Macro 3.134 89/09/18 AM C Alpha Micro 68K AMOSL 1.2 AM68K Asm 1.0 85/02/11 K20 D DECSYSTEM-20 TOPS-20 MACRO-20 4.2 88/01/25 CK F Altos ACS68000 UNIX III,V C 5A189 93/06/30 CK F Dell PC Dell UNIX C 5A189 93/06/30 CK F Amdahl Mainframe UTSV, SVR2 C 5A189 93/06/30 CP A Delphi 100 CPM80 2.2 LASM 4.11 91/04/23 CP A Amstrad CPM80 2.2 LASM 4.11 91/04/23 RD2 D DG 800 RDOS BASIC - 87/03/26 APO C Apollo Aegis Pascal 2.9 89/05/07 CK F DG AViiON DG/UX C 5A189 93/06/30 CK F Apollo Aegis 9.x C 5A189 93/06/30 AOS D DG MV AOS,AOS/VS SP/Pascal - 85/02/08 CK F Apollo/HP SR10.0 C 5A189 93/06/30 CK F DG MV AOS/VS,-II C 5A189 93/06/30 CP A Apple II CPM80 2.2 LASM 4.11 91/04/23 DGM D DG MV AOS/VSMVUXC - 85/11/27 APP A Apple II DOS,ProDOS CROSS 3.87 90/12/05 RDO D DG Nova RDOS Fortran-5 - 84/09/14 UCA C Apple II UCSD p-Sys UCSD Pascal 1.0 86/04/08 AOS D DG S250 AOS Fortran-5 - 84/09/14 CK F Apple Macintosh AU/X C 5A189 93/06/30 CK F DIAB DS90 DNIX C 5A189 93/06/30 CK F Apple Macintosh Mac OS MPW C 09188 93/05/24 CK F Dolphin Triton UNIX SV/88 C 5A189 93/06/30 CN8 C Argos Pro PC CCPM86 ASM86 2.9 86/04/10 CK F Encore UMAX 4.x C 5A189 93/06/30 CK F AT&T 3B Series UNIX SVR3 C 5A189 93/06/30 CK F Encore UMAX V C 5A189 93/06/30 CK F AT&T 6300 PLUS UNIX SVR3 C 5A189 93/06/30 CP A Epson PX8 CPM80 2.2 LASM 4.11 91/04/23 CK F AT&T 6386 WGS UNIX SVR3 C 5A189 93/06/30 LUX C FACIT DTC/DTC2 ABC-DOS ABC-BASIC-II 4.11 90/07/13 CK F AT&T 7300 UNIXPCUNIX Sys V C 5A189 93/06/30 CN8 C Fallon 2000 CCPM86 ASM86 2.9 86/04/10 AR C Acorn Archimedes Arthur C 1.3 93/05/01 CP A Ferguson BigB.I CPM80 2.2 LASM 4.11 91/04/23 AR C Acorn Archimedes RISC_OS C 1.3 93/05/01 CK F Fortune 32:16 For:Pro2.1 C 5A189 93/06/30 ATA C Atari Home Comp. DOS Action! - 84/01/09 CK F FPS 500 FPX 4.1 C 5A189 93/06/30 UCP C Atari MEGA ST2 UCSD p-Sys Pascal 1.1 90/08/05 CN8 C FTS PCi CCPM86 ASM86 2.9 86/04/10 CK F Atari ST GEMDOS C 5A189 93/06/30 C86 C Fujitsu Micro16s CPM86 ASM86 2.9 85/09/23 CK F Atari ST MINIX ST C 5A189 93/06/30 C86 C Future FX20/FX30 CPM86 ASM86 2.9 86/04/10 CP A BigBoard II CPM80 2.2 LASM 4.11 91/04/23 GEC D GEC 4000 Series OS4000 MUM/SERC 3.9 89/05/07 B78 D Burroughs A-Series MCS/AS Algol 1.019 86/09/11 OS9 C Gimex III OS-9 C 1.5 85/09/20 CT C Burroughs B20 BTOS C 2.00 93/01/20 GM D Gould/SEL 32 MPX-32 Fortran 77+ 2.3 86/12/10 B68 D Burroughs B6800 CANDE Algol - 85/02/15 MS A GRiD Compass II MS-DOS MASM 3.10 91/03/18 B78 D Burroughs B7800 Burroughs Algol 1.019 86/09/11 H1 D Harris H100-1 VOS 4.1.1 Fortran-77 1.06 88/03/17 B79 D Burroughs B7900 Burroughs Algol 5.2 85/11/27 H8 D Harris 800 VOS Pascal,Asm - 85/02/11 CD3 D CDC Cyber NOS Fortran 5 3.4 88/05/10 CK F Harris NightHawk CX/UX 6.1 C 5A189 93/06/30 CYB D CDC Cyber NOS 2.2 Compass 1.0 86/04/17 CP A Heath H8 CPM80 2.2 LASM 4.11 91/04/23 NOS D CDC Cyber NOS 2.4 Compass 1.30 87/05/19 CP A Heath/Zenith-89 CPM80 2.2 LASM 4.11 91/04/23 CDC D CDC Cyber 170 NOS,NOS/BE Fortran-77 2.2 84/09/07 CP A Heath/Zenith-100 CPM85 LASM 4.11 91/04/23 CK F CDC Cyber 910 IRIX C 5A189 93/06/30 MS A Heath/Zenith-100 MS-DOS MASM 3.10 91/03/18 CK F Charles River UNOS C 5A189 93/06/30 MU D Honeywell MULTICS PL/I 2.0h 84/09/20 CIE C CIE 680/XX REGULUS C - 87/01/26 HD6 D Honeywell DPS6 GCOS6 C 2.01 91/06/03 CP A Cifer 1886 CPM80 LASM 4.11 91/04/23 HG D Honeywell DPS66 GCOS3,8 C 3.0 84/10/05 CP A Comart Communica CPM80 2.2 LASM 4.11 91/04/23 HC6 D Honeywell DPS8 CP-6 PL/6 1.00 88/01/28 C64 C Commodore 64 FORTH FORTH 1.5 85/02/08 HCP D Honeywell DPS8 CP-6 Pascal - 85/04/04 C64 C Commodore 64/128 DOS CROSS 2.27 92/09/30 HDP D Honeywell DPS8 GCOS/TSS B 1.1 85/03/21 CK F Commodore Amiga 3000UX C 5A189 93/06/30 HG D Honeywell DPS8 GCOS3,8 C 3.0 84/10/05 CK F Commodore Amiga Intuition C 5A189 93/06/30 HC6 D Honeywell DPS90 CP-6 PL/6 1.00 88/01/28 CK F Commodore Amiga UNIX SVR4 C 5A189 93/06/30 HCP D Honeywell DPS90 CP-6 Pascal - 85/04/04 CP A Compupro IF 3/4 CPM80 2.2 LASM 4.11 91/04/23 HL6 C Honeywell L6/10 MS-DOS MASM 1.20A 84/10/05 CVK D Computervision CGOS Fortran S 1.21 87/03/04 MS A HP Portable Plus MS-DOS MASM 3.10 91/03/18 PER D Concurrent 3200 OS/32 MT72 Fortran 1.0 87/03/04 MS A HP-110, 150 MS-DOS MASM 3.10 91/03/18 CK F Concurrent 3200 Xelos SV C 5A189 93/06/30 CP A HP-125 CPM80 2.2 LASM 4.11 91/04/23 CK F Concurrent 6xxx RTU 4,5,6 C 5A189 93/06/30 HPM D HP-1000 RTE6, RTEA F77 & Asm 1.99D 90/01/09 CK F Convergent CTIX C 5A189 93/06/30 HP2 C HP-264x - 8080ASM 1.2 87/10/09 CT C Convergent NGEN CTOS C 2.00 93/01/20 HP3 D HP-3000 MPE SPL - 91/10/21 CK F Convex ConvexOS C 5A189 93/06/30 HP3 D HP-3000 MPE C - 93/05/15 CP A CPT-85xx CPM80 2.2 LASM 4.11 91/04/23 CK F HP-9000 HP-UX C 5A189 93/06/30 CK F Cray X/MP, Y/MP UNICOS 6,7,8 C 5A189 93/06/30 HPB C HP-9000/200,/300 HP-BASIC HP BASIC 1.02 89/06/21 CR D Cray-1,Cray-XMP CTSS Fortran-77 - 85/02/08 CK F HP-9836CU HP-UX C 5A189 93/06/30 CK F Cray-2,Cray-3 CSOS C 5A189 93/06/30 HP9 C HP-9845 BASIC/SAM HP BASIC 1.00 86/10/07 CP A Cromemco CPM80 2.2 LASM 4.11 91/04/23 HP9 C HP-98xx UCSD p-Sys HP Pascal - 84/01/20 CN8 C Daisy PCi CCPM86 ASM86 2.9 86/04/10 HP8 C HP86 HP-BASIC HP BASIC 1.01 87/04/29 CK F DEC Alpha AXP OpenVMS C 5A189 93/06/30 HP8 C HP87 HP-BASIC HP BASIC 1.01 87/04/29 CK F DEC Alpha AXP OSF/1 C 5A189 93/06/30 IK B IBM 370 Series CICS/MVS Assembler 4.2.4 92/09/30 K12 D DEC PDP-8 OS/8 Fam. PAL-8 10g 90/09/13 IK B IBM 370 Series CICS/VSE Assembler 4.2.4 92/09/30 CK F DEC PDP-11 2.1x BSD C 5A189 93/06/30 MT2 D IBM 370 Series MTS PLUS - 86/11/03 K11 B DEC PDP-11 IAS 3.1 Macro-11 3.60 89/06/13 MTS D IBM 370 Series MTS Assembler - 84/01/06 MP B DEC PDP-11 MUMPS-11 MUMPS-1982 - 84/04/11 MTS D IBM 370 Series MTS Pascal 1.0 84/01/06

Page 26 Number 5, July 1993 Kermit News

Operating Program Program Released Operating Program Program Released Prefix Tape Machine System Language Version yy/mm/dd Prefix Tape Machine System Language Version yy/mm/dd

IK B IBM 370 Series MUSIC Assembler 4.2.3 92/09/30 CK F Olivetti PCs SCO UNIX C 5A189 93/06/30 GUT D IBM 370 Series MVS/GUTS Assembler - 85/04/05 MS A Olivetti PCs MS-DOS MASM, C 3.13 93/07/08 IK B IBM 370 Series MVS/ROSCOE Assembler 4.2.4 92/09/30 CN8 C Orion PCi CCPM86 ASM86 2.9 86/04/10 IK B IBM 370 Series MVS/TSO Assembler 4.2.4 92/09/30 CP A Osborne 1 CPM80 2.2 LASM 4.11 91/04/23 TS2 B IBM 370 Series MVS/TSO Pascal/VS,.. 2.3 87/10/01 UCM C PascalMicroengin UCSD p-Sys Pascal III.0 84/12/03 TSN B IBM 370 Series MVS/TSO ALP/Assem 1.1A 87/09/17 MS A PC/8088 & higher MS-DOS MASM, C 3.13 93/07/08 IK B IBM 370 Series MVSXA/TSOE Assembler 4.2.4 92/09/30 CK F PC/286 & higher Microport C 5A189 93/06/30 IK B IBM 370 Series VM/CMS Assembler 4.2.5 92/12/23 CK F PC/286 & higher SCO Xenix C 5A189 93/06/30 IK B IBM 370 Series VM/ESA/CMS Assembler 4.2.5 92/12/23 CK F PC/386 & higher 386BSD C 5A189 93/06/30 IK B IBM 370 Series VM/HPO/CMS Assembler 4.2.5 92/12/23 CK F PC/386 & higher BSDI/386 C 5A189 93/06/30 IK B IBM 370 Series VM/IS/CMS Assembler 4.2.5 92/12/23 CK F PC/386 & higher Coherent C 5A189 93/06/30 IK B IBM 370 Series VM/SP/CMS Assembler 4.2.5 92/12/23 CK F PC/386 & higher ESIX SVR3 C 5A189 93/06/30 IK B IBM 370 Series VM/XA/CMS Assembler 4.2.5 92/12/23 CK F PC/386 & higher Interactive C 5A189 93/06/30 MS A IBM compatibles MS-DOS MASM, C 3.13 93/07/08 CK F PC/386 & higher Linux/386 C 5A189 93/06/30 CS9 C IBM CS9000 CSOS Pascal - 92/09/10 CK F PC/386 & higher Microport C 5A189 93/06/30 CK F IBM Mainframe AIX 1.2 C 5A189 93/06/30 CK F PC/386 & higher MINIX/386 C 5A189 93/06/30 CK F IBM Mainframe AIX/ESA2.1 C 5A189 93/06/30 CK F PC/386 & higher MtXinuMach C 5A189 93/06/30 UCI C IBM PC UCSD p-Sys UCSD Pascal 0.1 84/05/23 CK F PC/486 & higher NeXTSTEP C 5A189 93/06/30 CC C IBM PC + clones ChineseDOS MASM 2.32A 91/09/09 CK F PC/386 & higher OS/2 1.x C 5A189 93/06/30 MX B IBM PC family MINIX C 4D 61 88/05/17 CK F PC/386 & higher OS/2 2.0 C 5A189 93/06/30 TP4 C IBM PC family PC-DOS Turbo Pascal 1.1a 88/04/15 CK F PC/386 & higher SCO ODT C 5A189 93/06/30 QK C IBM PC,XT,AT PC-DOS Turbo Pascal 3.1 88/12/14 CK F PC/386 & higher SCO UNIX C 5A189 93/06/30 QNX C IBM PC,XT,AT QNX 1.x C 1.0 85/09/23 CK F PC/386 & higher Solaris C 5A189 93/06/30 MS A IBM PC,XT,AT,jr PC-DOS MASM, C 3.13 93/07/08 CK F PC/386 & higher UnixWare C 5A189 93/06/30 MS A IBM PC family MS Windows MASM, C 3.13 93/07/08 UCP C Pecan UCSD p-Sys Pascal 1.1 90/08/05 WK A IBM PC family MS Windows Microsoft C - 91/10/19 PER D PerkinElmer 3200 OS/32 MT72 Fortran 1.0 87/03/04 PIC D IBM PC/XT,AT PICK DATA/BASIC 0.3 89/08/21 CK F PerkinElmer 3200 Xelos SV C 5A189 93/06/30 CK F IBM PS/2 AIX 1.2 C 5A189 93/06/30 PE7 D PerkinElmer 7000 IDRIS C 1.1 0 86/12/08 CK F IBM PS/2 OS/2 1.3 C 5A189 93/06/30 CP A PMC Micromate101 CPM80 2.2 LASM 4.11 91/04/23 CK F IBM PS/2 OS/2 2.00 C 5A189 93/06/30 PRI D Prime PRIMOS R2x PL/P 8.15 93/04/19 MS A IBM PS/2 Series PC-DOS MASM, C 3.13 93/07/08 CK F Pyramid 9810x(T) OSx C 5A189 93/06/30 CK F IBM RS/6000 AIX 3.x C 5A189 93/06/30 CP A Rair Black Box CPM80 2.2 LASM 4.11 91/04/23 CK F IBM RT PC 4.3BSDReno C 5A189 93/06/30 CP A RM380ZF, ZM CPM80 2.2 LASM 4.11 91/04/23 CK F IBM RT PC ACIS 4.x C 5A189 93/06/30 RM C RML 480Z ROS 2.x C 1.22 86/11/03 CK F IBM RT PC AIX 2.x C 5A189 93/06/30 RM C RML Nimbus MS-DOS? C 1.22 86/11/03 VME D ICL 2900 VME S3 1.01 87/07/14 CP A Sanyo 1100 MBC CPM80 2.2 LASM 4.11 91/04/23 CK F ICL DRS3000,6000 DRS/NX C 5A189 93/06/30 MS A Sanyo 550 MBC MS-DOS MASM 2.30 88/05/16 CN8 C ICL PC 2,Quattro CCPM86 ASM86 2.9 87/05/17 CP A ScreenTyper CPM80 2.2 LASM 4.11 91/04/23 PQ C ICL/Perq Perq OS Pascal 2.0 84/12/04 CK F Sequent DYNIX C 5A189 93/06/30 CK F Integr.Solu.VS8 ISI 4.2BSD C 5A189 93/06/30 CK F Sequent DYNIX/ptx C 5A189 93/06/30 MS A Intel 300 Series iRMX-286 MASM/ASM862.30 88/05/02 CK F Silicon Graphics IRIX C 5A189 93/06/30 CK F Intel 302 Bell Tech C 5A189 93/06/30 QL2 C Sinclair QL QDOS BCPL - 87/05/15 RMX C Intel 86,286 RMX 1.0 PL/M 1.0 85/10/25 QLK C Sinclair QL QDOS C 1.10 87/05/15 I86 C Intel 86/380 iRMX-86 PL/M 2.3 85/09/23 CK F Solbourne OS/MP C 5A189 93/06/30 IRM C Intel 86/380 iRMX-86 PL/M 2.41 87/03/04 CK F Sony NEWS NEWS-OS C 5A189 93/06/30 MD C Intel MDS ISIS PL/M - 87/04/06 UN D Sperry 1100 Exec Assembler 2.5 86/09/03 CK F Intergraph Clipper CLIX C 5A189 93/06/30 UN D Sperry 1100 Exec NOSC Pascal 2.0 84/10/08 CP A Ithaca Intersys CPM80 2.2 LASM 4.11 91/04/23 CK F Sperry 5000 UNIX SVR3 C 5A189 93/06/30 UCJ C J Loebl Magiscan2 UCSD p-Sys UCSD Pascal - 86/06/23 CK F Sperry 5000 UTS V C 5A189 93/06/30 CP A Kaypro II CPM80 2.2 LASM 4.11 91/04/23 SP9 D Sperry 90/60 VS9 Assembler - 86/04/09 CP A Kaypro 4 CPM80 2.2 LASM 4.11 91/04/23 CK F Stardent 1520 UNIX SVR3 C 5A189 93/06/30 M2 C Lilith Worksta. Medos Modula-2 1.0 87/05/17 CK F Sun, all models Solaris 1,2 C 5A189 93/06/30 LM C LMI Lispmachine LMI-Lambda ZETALISP 1.0 85/09/12 CK F Sun, all models SunOS 3,4,5 C 5A189 93/06/30 CP A Lobo Max-80 CPM80 2.2 LASM 4.11 91/04/23 CP A Superbrain CPM80 2.2 LASM 4.11 91/04/23 LUX C Luxor ABC-80 ABC-DOS Z80 Asm 1.0 90/07/13 LM C Symbolics 36xx Lisp ZETALISP 1.0 85/09/12 LUX C Luxor ABC-80x ABC-DOS ABC-BASIC-II 4.11 90/07/13 TAN D Tandem Nonstop Guardian TAL 1.0 86/04/08 CK F Luxor ABC-9000 DNIX C 5A189 93/06/30 TA1 C Tandy 100 Tandy 100 BASIC 1984 90/10/07 MBF D MAI Basic Four BOSS/VS BASIC BB86 1.0 88/04/11 TA2 C Tandy 2000 MS-DOS MASM 1.20 84/02/16 CK F Masscomp RTU 4.0+ C 5A189 93/06/30 CK F Tandy Model 16 Xenix 3.0 C 5A189 93/06/30 CP A Merlin M2215 CPM80 2.2 LASM 4.11 91/04/23 C86 C Tektronix 4170 CPM86 ASM86 2.9 84/12/03 PIC D MicroDataREALITY PICK DATA/BASIC 0.3 89/08/21 CK F Tektronix 4xxx UTek C 5A189 93/06/30 CP A Micromint SB180 CPM80 2.2 LASM 4.11 91/04/23 CK F Tektronix 6130 UTek C 5A189 93/06/30 CK F MIPS System RISC/os C 5A189 93/06/30 CK F Tektronix XD88 UTek C 5A189 93/06/30 CK F Modcomp 9730 Real/IX C 5A189 93/06/30 CP A Telcon Zorba CPM80 2.2 LASM 4.11 91/04/23 MOD D Modcomp Classic MAX IV Fortran/ASM A.0 87/01/26 CP A Teletek CPM80 2.2 LASM 4.11 91/04/23 CK F Modcomp Realstar Real/IX C 5A189 93/06/30 UCT C Terak UCSD p-Sys UCSD Pascal - 84/04/11 CP A MorrowDecisionI CPM80 2.2 LASM 4.11 91/04/23 TI9 D TI 990 DX10 Pascal 1.0 87/07/10 CP A MorrowMicroDecI CPM80 2.2 LASM 4.11 91/04/23 EXP C TI Explorer LISP Common Lisp 1.0 87/03/04 FL C Motorola 6809 Flex Assembler - 86/02/14 MS A TI Professional MS-DOS MASM 2.29 86/05/28 FL2 C Motorola 6809 FLEX-09 C 3.0 87/03/04 CP A Torch Unicorn 5 CPM80 2.2 LASM 4.11 91/04/23 CK F Motorola Delta SV/68 R3x C 5A189 93/06/30 CK F Tri Star Flash ESIX C 5A189 93/06/30 CK F Motorola Delta SV/88 R3,4 C 5A189 93/06/30 CO C TRS-80 CoCo DOS EDTASM 1.1 85/03/21 NCR D NCR 9800-4 VE4.0 C 4E 72 90/07/13 OS9 C TRS-80 CoCo OS-9 C 1.5 85/09/20 CP A NCR Decisionmate CPM80 2.2 LASM 4.11 91/04/23 TRS C TRS-80 I and III TRSDOS M80 3.5 84/08/08 CK F NCR System 3000 UNIX SVR4 C 5A189 93/06/30 CP A TRS-80 Model II CPM80 2.25 LASM 4.11 91/04/23 CK F NCR Tower 1632 UNIX SVR2 C 5A189 93/06/30 TR2 C TRS-80 Model II TRSDOS Assembler 1.2 87/03/26 CK F NCR Tower 32 UNIX SVR3 C 5A189 93/06/30 CP A TRS-80 Model 4 CPM80 2.2 LASM 4.11 91/04/23 C86 C NEC APC CPM86 ASM86 2.9 84/12/03 M4 C TRS-80 Model 4 TRSDOS ASM 5.2 86/10/29 MS A NEC APC MS-DOS MASM 2.29 86/05/28 UM C UMicro U-MAN1000 CP/M-68K C and Asm - 86/04/10 MS A NEC APC III MS-DOS MASM 2.30 88/03/21 CK F UNISYS 5000 UNIX SVR3 C 5A189 93/06/30 MS A NEC PC9801 MS-DOS MASM 3.10 91/04/18 CK F UNISYS 5000 UTS V C 5A189 93/06/30 CK F NeXT NeXT OS C 5A189 93/06/30 UAS D UNISYS A-Series MCS/AS Algol 1.041 90/07/13 CK F Nixdorf Targon31 TOS C 5A189 93/06/30 CP A USmicroSalesS100 CPM80 2.2 LASM 4.11 91/04/23 CP A Nokia MikroMikko CPM80 2.2 LASM 4.11 91/04/23 PIC D VAX/Ultimate PICK DATA/BASIC 0.3 89/08/21 ND D Norsk Data 10,.. SintranIII ND-Pascal 3.1b 85/06/24 CP A Vector Graphics CPM80 2.2 LASM 4.11 91/04/23 CK F Norsk Data 88/17 UNIX SV/88 C 5A189 93/06/30 C86 C Victor/Sirius 1 CPM86 ASM86 2.9 86/07/07 CP A Northstar CPM80 2.2 LASM 4.11 91/04/23 MS A Victor/Sirius 1 MS-DOS MASM 3.10 91/03/18 CP A Ohio Scientific CPM80 2.2 LASM 4.11 91/04/23 CP A Video Genie CPM80 2.2 LASM 4.11 91/04/23 CK F OkiStation 7300 UNIX SVR4 C 5A189 93/06/30 MS A Wang PC, APC MS-DOS MASM 2.31 88/08/13 CK F Olivetti CP 486 UNIX SVR4 C 5A189 93/06/30 CP A Xerox 820 CPM80 2.2 LASM 4.11 91/04/23 CK F Olivetti LSX30xx X/OS C 5A189 93/06/30

Kermit News KERMIT ORDER FORM, SIDE 1 Number 5, July 1993

Prices, terms, and items are subject to change. If this form is dated more than 6 months prior, please contact us for new information. Please order carefully since we CANNOT refund or exchange items. Prices are in US dollars ($), first price for North America / second price for shipping outside North America (unless you pay shipping). ______________________________________________________________________________________________________________ 9-TRACK MAGNETIC TAPE. Price: $100 / $135 per tape:

ANSI TAR OS ANSI TAR OS ANSI TAR OS Tape A: Tape C: Tape E: Tape B: Tape D: See below for C-Kermit . . .

9-TRACK TAPE SUBTOTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ ______________________________________________________________________________________________________________ TAPE CARTRIDGES. Price: $150 / $185. 8MM QIC TK50

Contents of Tapes A, B, and E: Contents of Tapes C, D, and E:

TAPE CARTRIDGE SUBTOTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ ______________________________________________________________________________________________________________ MS-DOS KERMIT IBM PC/PS2 MS-DOS Kermit software with book Using MS-DOS Kermit, $34.95 / $45:

5.25-inch 3.5-inch: . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

IBM PC/PS2 MS-DOS Kermit utilities and technical documentation: $35 / $40:

5.25-inch 3.5-inch: . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

MS-DOS IBM PC/PS2 Kermit source code, $60 / $68:

5.25-inch 3.5-inch: . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

Crynwr (formerly Clarkson) packet drivers. For the IBM PC family on DOS diskettes:

Binaries and Docs, $35 / $40: 5.25-inch 3.5-inch . . . . . . . . . . . . . . . . . . . . . . . . . $__________ Source Code, $60 / $68: 5.25-inch 3.5-inch . . . . . . . . . . . . . . . . . . . . . . . . . $__________ ______________________________________________________________________________________________________________ C-KERMIT 5A, includes book Using C-Kermit:

9-Track Tape, $135 / $170, Format: ANSI, TAR . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ TK50 cartridge, DEC VMS / OpenVMS BACKUP format, $185 / $220 . . . . . . . . . . . . . . . . . . . . . . . . . $__________ Quarter-Inch Cartridge (QIC), UNIX TAR format, $185 / $220 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ 8mm EXABYTE cartridge, UNIX TAR format, $185 / $220 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ Source code on DOS-format diskettes, $100 / $115: 5.25-inch, 3.5-inch: . . . . . . . . . . . . . . . . . $__________

Binaries on DOS-format diskettes, Using C-Kermit book included, $45 / $50 each: 3.5" 5.25"

C-Kermit for OS/2 1.xx, 16-bit . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ C-Kermit for OS/2 2.00, 32-bit . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ C-Kermit for OS-9/68000 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ C-Kermit for Commodore Amiga . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ C-Kermit for Atari ST . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

______________________________________________________________________________________________________________ MACINTOSH KERMIT

Mac Kermit 0.9(40) 1988 release, 3.5-inch, $25 / $30 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ Mac Kermit 0.99(???) latest prerelease, 3.5-inch, $25 / $30 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

______________________________________________________________________________________________________________ LITERATURE

Book: Kermit, A File Transfer Protocol: $29.95 / $35 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ Book: Using C-Kermit (without software): $34.95 / $45 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ Book: Using MS-DOS Kermit: $34.95 / $45 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________ Technical paper, Recent Kermit Protocol Extensions: $15 / $25 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

Kermit Digest volumes, $15 / $25 per year:

This year Last 2 years Last 3 years Last 4 years . . . . . . . . . . . . . . . . . . . . . . $__________

Manuals for Kermit programs: $10 / $13 each:

IBM 370 Apple II PDP-11 CP/M-80 . . . . . . . . . . . . . . . . . . . . . . . . $__________

SIDE 1 SUBTOTAL (please complete side 2 also) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

Number 5, July 1993 KERMIT ORDER FORM, SIDE 2 Kermit News

Shipping by UPS or post is included in the price. Please do not add sales tax.

SUBTOTAL from Side 1: . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

Voluntary tax-deductible donation (help support the Kermit effort) : . . . . . . . . . . . . $__________

USA, CANADA, AND MEXICO ONLY:

For PRIORITY HANDLING and NEXT-DAY SHIPMENT, add $30: . . . . . . . . . . . $__________

A. TOTAL MATERIALS, DONATION, AND SHIPPING: . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

Please complete ONE of the numbered sections, 1, 2, or 3, and then fill in your shipping information.

1. PAYMENT BY CREDIT CARD

MasterCard Visa AMOUNT OF YOUR PAYMENT (Line A above): $__________

Card Number ______________________________________________ Expiration Date ____________________________________

Signature __________________________________________________ Today’s Date _______________________________________

2. PREPAYMENT BY CHECK

Please enclose a check for the total amount, payable in US dollars. PLEASE DO NOT MAKE ELECTRONIC BANK TRANSFERS OR SEND INTERNATIONAL POSTAL COUPONS. Make your check payable to:

Columbia University Kermit Distribution If your check is not drawn on a US bank, please add a $35 check-cashing fee: . . . . . . . $__________

TOTAL AMOUNT OF YOUR CHECK: . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . $__________

3. PURCHASE ORDERS

B. Amount from Line A above: $__________ C. Add $25 order processing fee: $__________ D. If your check will not be drawn on a US bank, add $35 check-cashing fee: $__________ TOTAL, Lines B, C, and D. Please enclose your purchase order for this amount: . . . . . . . . . . . . . . . . . . $__________

SHIPPING INFORMATION (Do not use Post Office Box for UPS or Federal Express):

Name:_____________________________________ Organization: ________________________________________________________

Address: ________________________________________________________________________________________________________

City:_________________________State or Province:______________Zip or Postal Code: ___________________________________

Country:__________________________________________________Phone: ________________________________________________

If you want us to use your Federal Express account, please provide your account number and your signature:

Federal Express Account Number _________________________________________________________________________________

Signature _______________________________________________________________________________________________________

MAIL YOUR COMPLETED ORDER FORM TO:

Kermit Distribution, Department OP Columbia University Academic Information Systems 612 West 115th Street New York, NY 10025-7721 USA

Phone: +1 212 854-3703, FAX: +1 212 663-8202, E-Mail: kermit @columbia .edu. Sorry, we can’t respond by FAX.

Thank you!

Directory

Postal Address:

Kermit Development and Distribution Columbia University Academic Information Systems 612 West 115th Street New York, NY 10025-7721 USA

Staff:

Christine M. Gianone, Manager Max Evarts Andy Newcomb

Telephone:

Ordering Information: +1 212 854-3703 Technical Support: +1 212 854-5126 Fax: +1 212 663-8202

Networks:

BITNET/EARN/CREN: KERMIT@CUVMA Internet: kermit@columbia.edu