The Windows port of frontpanel library was done by Stefano Bodrato, great job, many thanks for this!

Stefano can be reached at stefano_bodrato@hotmail.com.

To start the machines and boot them with CP/M change to the directories and run the inluded .bat scripts. In the bin direcory you will also find z80asm.exe, which you can use to assemble some Z80 source on your Windows system.

The IMSAI emulation comes with a 3D and a 2D model, by default the 3D model is active. Run the batch scripts setup2d.bat or setup3d.bat to change this. Also in the 3D model you can switch to the 2D view by pressing the v-key in the front panel window.

You can download instruction manuals for operating the machines at the z80pack project page: http://www.autometer.de/unix4fun/z80pack/

You also can download much more CP/M software from there to run on the machines. Please be aware that the packages there are build for UNIX, and so they include UNIX shell scripts to mount disks and start emulations. Just copy the disk image files into the disks\library directory for the machine and use the already included .bat files as examples, how to build your own ones.

Have fun with this,
March 2014, Udo Munk
