{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":68,"n_cols":59,"rows_kept":68,"cut":false,"hidden":false,"merged":[]}
["Wang 360E",null,"Keyboard latch/decode",null,null,null,null,"Master Clock/Timing",null,null,null,null,"System State FFs",null,null,null,null,"B-Counter, Major Cycles",null,null,null,null,"B-State: 7/8/10",null,null,null,null,"B-State: 6/9",null,null,null,null,"B-State: 3/4/5",null,null,null,null,"B-State: 1/2",null,null,null,null,"B-State: 0/1",null,null,null,null,"R-Counter Minor Cycles",null,null,null,null,"T-Counter Minor Cycles"]
[null,"ok",514,"#1","ok",null,"ok",519,"#2","ok",null,"ok",520,"#3","ok",null,"ok",516,"#4","ok",null,"ok",508,"#5","ok",null,"ok",507,"#6","ok",null,"ok",506,"#7","ok",null,"ok",505,"#8","ok",null,"ok",504,"#9","ok",null,"ok",517,"#10","ok",null,"ok",515,"#11","ok"]
[null,"A","KB2","KB8",1,null,"A","-5.1vz","-5.1vz",1,null,"A","B4","!(LG)",1,null,"A","!(B8)","Treset",1,null,"A","OFon","ACG",1,null,"A","XG2","SD1",1,null,"A","DE0","r15",1,null,"A","SD0","b41",1,null,"A","SC0","b0b",1,null,"A","!(R8)","!(R8)",1,null,"A","!(T8)","!(T1)",1,null,null,"Notes for Use"]
[null,"B","KB4","K8",2,null,"B","Rg","Rg",2,null,"B","B2","!(B1)",2,null,"B","B8","!(B1)",2,null,"B","S","PS",2,null,"B","H0off","SC2",2,null,"B","b4","AD1",2,null,"B","SD7","r1",2,null,"B","DPoff","B4S",2,null,"B","R8","!(R1)",2,null,"B","T8","Tpulse",2,null,null,"Double-click a signal name to trace it"]
[null,"C","K4","K2",3,null,"C","n0","SW1",3,null,"C","B8","ACGP",3,null,"C","!(B4)","B4",3,null,"C","r15","PSG",3,null,"C","!(T1)","!(S)",3,null,"C","r0","!(AD8)",3,null,"C","!(H0)","K!8!2!1",3,null,"C","DP","!(k10S)",3,null,"C","!(R4)","Rpulse",3,null,"C","T4","!(T4)",3]
[null,"D","!(K4)","!(K8)",4,null,"D","!(SW1)","!(SW1)",4,null,"D","B1","!(B2)",4,null,"D","Bpulse","Bpulse",4,null,"D","XG1","k1",4,null,"D","r0","b40",4,null,"D","CP","E4",4,null,"D","RW","!(K!8!2)",4,null,"D","b01b","SD1",4,null,"D","!(R2)","R4",4,null,"D","!(T2)","!(T2)",4,null,null,"Colour Code"]
[null,"E","!(YT1)","!(K2)",5,null,"E","n1","n1",5,null,"E","n0","!(DP)",5,null,"E","B1","!(B2)",5,null,"E","CA","CP",5,null,"E","SD0","b4",5,null,"E","!(E2)","!(DE0)",5,null,"E","BS","CID",5,null,"E","H0off","!(k3)",5,null,"E","R1","R1",5,null,"E","T2","T2",5,null,null,"Red - signal generated"]
[null,"F","k1","KB1",6,null,"F","!(p0)","QH",6,null,"F","n1","DPoff",6,null,"F","N/C","S",6,null,"F","CID","CIR",6,null,"F","BS","b44",6,null,"F","H1on","H0on",6,null,"F","!(k10s)","H1",6,null,"F","SB5","!(K8)",6,null,"F","R2","R2",6,null,"F","T1","!(b51)",6,null,null,"Green - signal used"]
[null,"H","b9","k7",7,null,"H","p0","OF",7,null,"H","DP","DPon",7,null,"H","B2","B2",7,null,"H","H1off","SW1",7,null,"H","CID","!(Q)",7,null,"H","r14","b44",7,null,"H","r0","GR",7,null,"H","!(R2)","Q",7,null,"H","r2","r2",7,null,"H","t2","t2",7,null,null,"Grey - indetermined"]
[null,"J","!(E1)","Y1K",8,null,"J","p1","Rreset",8,null,"J","DA","ACG",8,null,"J","b4","b4",8,null,"J","H1","SW2",8,null,"J","H0on","E4",8,null,"J","!(r15)","RW",8,null,"J","H1off","CP",8,null,"J","!(R4)","!(S)",8,null,"J","r1","r1",8,null,"J","t1","t1",8,null,null,null,"Double click colours to change"]
[null,"K","!(k7)","!(YT2)",9,null,"K","!(p01)","!(p01)",9,null,"K","H1","RCGP",9,null,"K","b3","b5",9,null,"K","r14","r4",9,null,"K","t13","r14",9,null,"K","!(r14)","!(r0)",9,null,"K","b2","K!8!42",9,null,"K","OFon","!(Q)",9,null,"K","r3","r3",9,null,"K","t3","T16",9]
[null,"L","E1K","Y2K",10,null,"L","p2","p2",10,null,"L","H0","H1off",10,null,"L","b8","b7",10,null,"L","!(H1)","K10S",10,null,"L","XG1","ERC",10,null,"L","K2","PSG",10,null,"L","H0off","LK",10,null,"L","!(R8)","b1b",10,null,"L","r7","r7",10,null,"L","!(T16)","t7",10]
[null,"M","K!8!41","!(YT4)",11,null,"M","p3","p3",11,null,"M","H1on","H1on",11,null,"M","!(r0)","!(r0)",11,null,"M","r0","BG1",11,null,"M","!(ERC)","RCG",11,null,"M","SD7","!(K4)",11,null,"M","b43","SD1",11,null,"M","H0","r0",11,null,"M","r4","r4",11,null,"M","!(r0)","!(p0)",11]
[null,"N","!(YT8)","Y4K",12,null,"N","!(p2)","KBC",12,null,"N","N/C","N/C",12,null,"N","!(b51)","!(b51)",12,null,"N","SGG","BG4",12,null,"N","LK","b2",12,null,"N","H1","!(K!82)",12,null,"N","H0","!(Q)",12,null,"N","SGG","DG2",12,null,"N","r5","Rreset",12,null,"N","t5","t5",12]
[null,"P","E2K","Y8K",13,null,"P","p4","RUN",13,null,"P","N/C","N/C",13,null,"P","b6","b6",13,null,"P","b7","!(Q)",13,null,"P","stop","H1on",13,null,"P","b3","AD8",13,null,"P","!(LK)","!(K!8!2!1)",13,null,"P","t0","RST",13,null,"P","!(r1234)","!(p0)",13,null,"P","CL_ALL","CL_ALL",13]
[null,"R","K!81","KB16",14,null,"R","!(p34)","!(KE)",14,null,"R","H0off","H0off",14,null,"R","b50","b1",14,null,"R","!(r15)","!(p01)",14,null,"R","!(AD0)","!(E2)",14,null,"R","!(H0)","!(AD1)",14,null,"R","!(S)","!(DE0)",14,null,"R","RW","XG2",14,null,"R","r9","Rg",14,null,"R","T4S","t9",14]
[null,"S","!(k3)","K16",15,null,"S","!(p4)","KE",15,null,"S","H0on","H0on",15,null,"S","Breset","BS",15,null,"S","!(DE0)","SW3",15,null,"S","T1","b6",15,null,"S","BS","CA",15,null,"S","!(k3)","K!82",15,null,"S","T4S","XG1",15,null,"S","!(S)","S",15,null,"S","Treset","TG",15]
[]
[null,"A","-11v","k3",1,null,"A","-11v","-11v",1,null,"A","-11v","-11v",1,null,"A","-11v","-11v",1,null,"A","-11v","spare",1,null,"A","-11v","H1off",1,null,"A","-11v","SD3",1,null,"A","-11v",null,1,null,"A","-11v","SC2",1,null,"A","-11v","-11v",1,null,"A","-11v","-11v",1]
[null,"B","+11v","E4K",2,null,"B","+11v","+11v",2,null,"B","+11v","+11v",2,null,"B","+11v","+11v",2,null,"B","SBLC","stop",2,null,"B","CR","H0",2,null,"B","stop","OFon",2,null,"B","!(H1)","H1on",2,null,"B","QH","S",2,null,"B","+11v","+11v",2,null,"B","+11v","+11v",2]
[null,"C","+-0v","!(K16)",3,null,"C","+-0v","+-0v",3,null,"C","+-0v","+-0v",3,null,"C","+-0v","+-0v",3,null,"C","SC0","K4",3,null,"C","AD0","TG",3,null,"C","H1off","K!82",3,null,"C","H0on","!(AD0)",3,null,"C","BS","r15",3,null,"C","+-0v","+-0v",3,null,"C","+-0v","+-0v",3]
[null,"D","K!8!4","LK",4,null,"D","!(RW)","ERC",4,null,"D","!(H0)","DAon",4,null,"D","!(b1c)","b01b",4,null,"D","!(r0)","!(K8)",4,null,"D","r15","b50",4,null,"D","CID","SBLC",4,null,"D","b40","K!8!41",4,null,"D","!(KE)","!(K!8!4!2)",4,null,"D","r8","r0",4,null,"D","stop_pulse","stop_pulse",4]
[null,"E","K!82","!(K!8!4)",5,null,"E","b42","!(H0)",5,null,"E","!(H1)","!(b1c)",5,null,"E","N/C","N/C",5,null,"E","!(AD0)","b1a",5,null,"E","CP","H1",5,null,"E","XG1","K!8!4",5,null,"E","B4S","K!8!4!2",5,null,"E","CP","b0a",5,null,"E","r11","spare NOR",5,null,"E","t10","Breset",5]
[null,"F","!(E8)","!(K!82)",6,null,"F","!(RDdv)","H1",6,null,"F","!(DA)","!(AD0)",6,null,"F","!(b50)","B4S",6,null,"F","H1on","RW",6,null,"F","k3","RW",6,null,"F","CR","!(RW)",6,null,"F","!(r15)","K!81",6,null,"F","DE0","K!8!4!2",6,null,"F","!(r0)","spare NOR",6,null,"F","STOP","STOP",6]
[null,"H","K!82!1","E8K",7,null,"H","!(WRdv)","!(b1c)",7,null,"H","RCG","OFon",7,null,"H","b9","b1c",7,null,"H","SD0","SC1",7,null,"H","!(H0)","QH",7,null,"H","LG","!(K8)",7,null,"H","K!82!1","K!8!2",7,null,"H","!(RST)","!(K!8!2!1)",7,null,"H","r15","r10",7,null,"H","t11","t11",7]
[null,"J","K!8!42","!(k2)",8,null,"J","!(ERC)","Q",8,null,"J","!(r0)","AD0",8,null,"J","b2","!(b01b)",8,null,"J","!(r1234)","SD1",8,null,"J","!(K4)","SBLC",8,null,"J","S","!(S)",8,null,"J","b44","k10S",8,null,"J","SD6","!(r15)",8,null,"J","r14","!(r15)",8,null,"J","t13","LG",8]
[null,"K","!(LK)","k2",9,null,"K","WRdv","!(S)",9,null,"K","!(P0)","OF",9,null,"K","b10","b0a",9,null,"K","!(SW1)","GR",9,null,"K","!(K2)","K!8!41",9,null,"K","SD0","GR",9,null,"K","r15","Q",9,null,"K","DA","!(H0)",9,null,"K","r13","!(r14)",9,null,"K","t8","t8",9]
[null,"L","K!8!4!2","!(K!8!4!2)",10,null,"L","KBI","!(b2)",10,null,"L","!(OF)","k10S",10,null,"L","!(b2)","b1b",10,null,"L","b10","b3",10,null,"L","k7","b5",10,null,"L","b5","r1",10,null,"L","!(r0)","K8",10,null,"L","SD0","DE15",10,null,"L","stop_pulse","KB",10,null,"L","t6","LK",10]
[null,"M","!(E4)","!(K!8!2!1)",11,null,"M","!(KB)","!(Q)",11,null,"M","PSP","PSG",11,null,"M","b1a","b0b",11,null,"M","RST","b41",11,null,"M","!(k7)","b0a",11,null,"M","H0off","!(H1)",11,null,"M","CA","b42",11,null,"M","TG","!(DA)",10,null,"M","K2","K1",11,null,"M","t4","!(RST)",11]
[null,"N","!(E2)","!(K1)",12,null,"N","b40","S",12,null,"N","!(RST)","OFa",12,null,"N","b0","!(b1)",12,null,"N","CR","XG2",12,null,"N","b9","DAR",12,null,"N","H0","!(AD0)",12,null,"N","SGC","K!8!4",12,null,"N","K!8!2!1","SD3",10,null,"N","K8","K4",12,null,"N","t14","t14",12,null,null,"Copyright"]
[null,"P","K!8!2!1","!(K!8!2)",13,null,"P","b43","!(r0)",13,null,"P","!(PS)","!(k10S)",13,null,"P","!(b0)","!(K16)",13,null,"P","!(S)","QH",13,null,"P","Q","!(r0)",13,null,"P","k7","CIR",13,null,"P","b1c","XG2",13,null,"P","!(DE15)","stop",10,null,"P","H0","K16",13,null,"P","RST","RST",13,null,null,"This work is copyright ATC 2014"]
[null,"R","K1","K!8!2",14,null,"R","SPARE","b41",14,null,"R","LG","K10S",14,null,"R","K16","!(K!8!4)",14,null,"R","BS","b8",14,null,"R","S","!(T16)",14,null,"R","SD1","!(LG)",14,null,"R","k3","OFon",14,null,"R","b1a","DPon",10,null,"R","KE","KE",14,null,"R","t0","N/C",14,null,null,"It may be distributed provided that no"]
[null,"S","RCGP","ACGP",15,null,"S","KB","b44",15,null,"S","PS","DAR",15,null,"S","!(KE)","K!8!4",15,null,"S","SD7","DE0",15,null,"S","SB3","SC0",15,null,"S","K!8!2","RCG",15,null,"S","!(K!82)","XG1",15,null,"S","H0on","DAon",10,null,"S","r12","r6",15,null,"S","t12","t12",15,null,null,"charge is made and this copyright is intact"]
[]
[null,null,"E8K","Y8K",null,null,null,"T1","E1"]
[null,null,"Log Generator #3",null,null,null,null,"Log Generator #2",null,null,null,null,"Log Generator #1",null,null,null,null,"B-Switch",null,null,null,null,"4 bit Parallel BCD Adder",null,null,null,null,"Data Switch, Buffer Amps",null,null,null,null,"G-Reg, Core Current Srces",null,null,null,null,"8 line XY Core Drivers",null,null,null,null,"8 line XY Core Drivers",null,null,null,null,"8x16x4 Core, Sense & Inhib",null,null,null,null,"Mem Reg Control"]
[null,null,503,"#12",null,null,null,502,"#13",null,null,null,501,"#14",null,null,"ok",518,"#15","ok",null,"ok",512,"#16","ok",null,"ok",511,"#17","ok",null,"ok",513,"#18","ok",null,"ok",510,"#19","ok",null,"ok",510,"#20","ok",null,"ok",527,"#21","ok",null,"ok",540,"#22","ok"]
[null,"A",null,null,1,null,"A",null,null,1,null,"A",null,null,1,null,"A","BG4","G4",1,null,"A","AD2","!(Ab1)",1,null,"A","!(DG1)","R1",1,null,"A","REG-6v","REG-6v",1,null,"A","REG-6v","REG-6v",1,null,"A","REG-6v","REG-6v",1,null,"A","Z6","Z0",1,null,"A","REG-6v",null,1]
[null,"B",null,null,2,null,"B",null,null,2,null,"B",null,null,2,null,"B","BG8","G8",2,null,"B","E1","!(AD2)",2,null,"B","CG1","R2",2,null,"B","REG+5.7v","REG+5.7v",2,null,"B","REG+5.7v","REG+5.7v",2,null,"B","REG+5.7v","REG+5.7v",2,null,"B","REG+5.7v",null,2,null,"B","REG+5.7v",null,2]
[null,"C",null,null,3,null,"C",null,null,3,null,"C",null,null,3,null,"C","BG2","G2",3,null,"C","!(AD1)","!(AD1)",3,null,"C","TP1","R4",3,null,"C","+-0vCORE","+-0vCORE",3,null,"C","+-0vCORE","+-0vCORE",3,null,"C","+-0vCORE","+-0vCORE",3,null,"C","+-0vCORE",null,3,null,"C","+-0vCORE",null,3]
[null,"D",null,null,4,null,"D",null,null,4,null,"D",null,null,4,null,"D","SB3","G1",4,null,"D","!(CAS)","!(CAS)",4,null,"D","CG2","R8",4,null,"D","G1","G1",4,null,"D","!(YT2)","!(YT2)",4,null,"D","!(YT8)","!(YT8)",4,null,"D","!(DG1)","Z7",4,null,"D","Z7","!(RDdv)",4]
[null,"E",null,null,5,null,"E",null,null,5,null,"E",null,null,5,null,"E","!(SB4)","!(R1)",5,null,"E","!(E1)","!(E1)",5,null,"E","SC0","!(R1)",5,null,"E","!(G1)","!(G1)",5,null,"E","!(YT1)","!(YT1)",5,null,"E","!(YT4)","!(YT4)",5,null,"E","!(DG2)","Z5",5,null,"E","Z5","WRdv",5]
[null,"F",null,null,6,null,"F",null,null,6,null,"F",null,null,6,null,"F","BG1","!(R2)",6,null,"F","Ab1","Ab1",6,null,"F","CG4","!(R2)",6,null,"F","E1","E1",6,null,"F","!(RDdv)","!(RDdv)",6,null,"F","!(RDdv)","!(RDdv)",6,null,"F","!(DG4)","X0",6,null,"F","Z3","Z1",6]
[null,"H",null,null,7,null,"H",null,null,7,null,"H",null,null,7,null,"H","SB4","!(R8)",7,null,"H","AD8","CAS",7,null,"H","CG8","!(R4)",7,null,"H","NIR","NIR",7,null,"H","X0","X0",7,null,"H","Y0","Y0",7,null,"H","!(DG8)","X1",7,null,"H","Zgate",null,7]
[null,"J",null,null,8,null,"J",null,null,8,null,"J",null,null,8,null,"J","!(Ab2)","!(R4)",8,null,"J","AD1","!(Ab2)",8,null,"J","TP2","!(R8)",8,null,"J","!(E1)","!(E1)",8,null,"J","X1","X1",8,null,"J","Y1","Y1",8,null,"J","X2","X3",8,null,"J",null,"CG1",8]
[null,"K",null,null,9,null,"K",null,null,9,null,"K",null,null,9,null,"K","SB5","Q",9,null,"K","E2","E2",9,null,"K","SC1","T1",9,null,"K","SE1","SE1",9,null,"K","X2","X2",9,null,"K","Y2","Y2",9,null,"K","X4","X5",9,null,"K",null,null,9]
[null,"L",null,null,10,null,"L",null,null,10,null,"L",null,null,10,null,"L","Ab2","r0",10,null,"L","TP9","TP9",10,null,"L","!(DG2)","T2",10,null,"L","G2","!(G2)",10,null,"L","X3","X3",10,null,"L","Y3","Y3",10,null,"L","X6","X7",10,null,"L",null,"Z4",10]
[null,"M",null,null,11,null,"M",null,null,11,null,"M",null,null,11,null,"M","!(CAS)","CA",11,null,"M","!(E2)","!(E2)",11,null,"M","SC2","T4",11,null,"M","N/C","E2",11,null,"M","!(XT1)","!(XT1)",11,null,"M","!(XT2)","!(XT2)",11,null,"M","Z3","Y0",11,null,"M","Z6","DAR",11]
[null,"N",null,null,12,null,"N",null,null,12,null,"N",null,null,12,null,"N","CID","!(CA)",12,null,"N","!(AD8)","Ab2",12,null,"N","DG1","T8",12,null,"N","SE2","!(E2)",12,null,"N",null,null,12,null,"N",null,null,12,null,"N","Z1","Y1",12,null,"N","RW","stop",12]
[null,"P",null,null,13,null,"P",null,null,13,null,"P",null,null,13,null,"P","!(SB1)","r1",13,null,"P","Ad2","TP10",13,null,"P","TP3","E1",13,null,"P","!(G4)","G4",13,null,"P","XT1","XT1",13,null,"P","XT2","XT2",13,null,"P","Y3","Y2",13,null,"P","!(Q)","SC0",13]
[null,"R",null,null,14,null,"R",null,null,14,null,"R",null,null,14,null,"R","SB1","!(p0)",14,null,"R","E4","!(Ab4)",14,null,"R","TP4","E2",14,null,"R","E4","!(DE0)",14,null,"R","CG1","CG1",14,null,"R","CG4","CG4",14,null,"R","Y5","Y4",14,null,"R","Q","stop_pulse",14]
[null,"S",null,null,15,null,"S",null,null,15,null,"S",null,null,15,null,"S","CAS","CR",15,null,"S","!(E4)","TP13",15,null,"S","DG4","E4",15,null,"S","!(E4)","DE0",15,null,"S","CG2","CG2",15,null,"S","CG8","CG8",15,null,"S","Y7","Y6",15,null,"S","SD1","SD7",15]
[]
[null,"A",null,null,1,null,"A",null,null,1,null,"A",null,null,1,null,"A","-11v","-11v",1,null,"A","-11v","-11v",1,null,"A","-11v","E8",1,null,"A","-11v","-11v",1,null,"A","-11v","-11v",1,null,"A","-11v","-11v",1,null,"A","-11v",null,1,null,"A","-11v",null,1]
[null,"B",null,null,2,null,"B",null,null,2,null,"B",null,null,2,null,"B","+11v","+11v",2,null,"B","+11v","+11v",2,null,"B","+11v","K1",2,null,"B","+11v","+11v",2,null,"B","+11v","+11v",2,null,"B","+11v","+11v",2,null,"B","+11v",null,2,null,"B","+11v",null,2]
[null,"C",null,null,3,null,"C",null,null,3,null,"C",null,null,3,null,"C","+-0v","+-0v",3,null,"C","+-0v","+-0v",3,null,"C","+-0v","K2",3,null,"C","+-0v","+-0v",3,null,"C","+-0v","+-0v",3,null,"C","+-0v","+-0v",3,null,"C","+-0v",null,3,null,"C","+-0v",null,3]
[null,"D",null,null,4,null,"D",null,null,4,null,"D",null,null,4,null,"D","spare","spare",4,null,"D","Ad4","Ab4",4,null,"D","!(p34)","K4",4,null,"D","GRP","SGG",4,null,"D","Xgate","Xgate",4,null,"D","Ygate","Ygate",4,null,"D","Z4","Z2",4,null,"D","XG2","!(K1)",4]
[null,"E",null,null,5,null,"E",null,null,5,null,"E",null,null,5,null,"E","C","b5",5,null,"E","E8","TP14",5,null,"E","SD1","K8",5,null,"E","!(p1)","!(p1)",5,null,"E","YT2","YT2",5,null,"E","YT8","YT8",5,null,"E","NIR",null,5,null,"E","Xgate","KE",5]
[null,"F",null,null,6,null,"F",null,null,6,null,"F",null,null,6,null,"F","CIR","b6",6,null,"F","Ad8","!(Ab8)",6,null,"F","!(DG4)","G1",6,null,"F","SGGP","SGGP",6,null,"F","XG2","N/C",6,null,"F","XG1","N/C",6,null,"F",null,null,6,null,"F","STN","KBC",6]
[null,"H",null,null,7,null,"H",null,null,7,null,"H",null,null,7,null,"H","!(Ab1)","G1L",7,null,"H","TP17","TP17",7,null,"H","SD6","G2",7,null,"H","SE4","SE4",7,null,"H","X4","X4",7,null,"H","Y4","Y4",7,null,"H",null,null,7,null,"H","CG2","SC2",7]
[null,"J",null,null,8,null,"J",null,null,8,null,"J",null,null,8,null,"J","Ab1","SBLC",8,null,"J","!(E8)","!(E8)",8,null,"J","TP6","G4",8,null,"J","GR","GR",8,null,"J","X5","X5",8,null,"J","Y5","Y5",8,null,"J",null,null,8,null,"J",null,"!(K4)",8]
[null,"K",null,null,9,null,"K",null,null,9,null,"K",null,null,9,null,"K","!(Ab4)","G.5L",9,null,"K","Ab8","Ab8",9,null,"K","!(DG8)","G8",9,null,"K","G8","G8",9,null,"K","X6","X6",9,null,"K","Y6","Y6",9,null,"K","SE4",null,9,null,"K","K2","K4",9]
[null,"L",null,null,10,null,"L",null,null,10,null,"L",null,null,10,null,"L","Ab4","K1",10,null,"L","TP18","TP18",10,null,"L","SD7","AD1",10,null,"L","!(G8)","!(G8)",10,null,"L","X7","X7",10,null,"L","Y7","Y7",10,null,"L","SE8",null,10,null,"L","BS","!(KE)",10]
[null,"M",null,null,11,null,"M",null,null,11,null,"M",null,null,11,null,"M","!(CP)","K2",11,null,"M","AD4","AD4",11,null,"M","TP8","AD2",11,null,"M","p1","!(DE15)",11,null,"M",null,null,11,null,"M",null,null,11,null,"M","SE1",null,11,null,"M","Z2","STM",11]
[null,"N",null,null,12,null,"N",null,null,12,null,"N",null,null,12,null,"N","!(Ab8)","!(K4)",12,null,"N","CA","CA",12,null,"N","DG2","AD4",12,null,"N","E8","DE15",12,null,"N","WRdv","WRdv",12,null,"N","WRdv","WRdv",12,null,"N",null,null,12,null,"N","Z0","K8",12]
[null,"P",null,null,13,null,"P",null,null,13,null,"P",null,null,13,null,"P","G2L","!(K1)",13,null,"P","!(AD4)","!(AD4)",13,null,"P","TP7","AD8",13,null,"P","!(E8)","!(RW)",13,null,"P","YT1","YT1",13,null,"P","YT4","YT4",13,null,"P","SE2",null,13,null,"P",null,"!(r0)",13]
[null,"R",null,null,14,null,"R",null,null,14,null,"R",null,null,14,null,"R","!(SB8)","Ab8",14,null,"R","!(CA)","!(CA)",14,null,"R","DG8","SD3",14,null,"R","ERP","N/C",14,null,"R",null,null,14,null,"R",null,null,14,null,"R","REG+5.1v",null,14,null,"R",null,"!(KB)",14]
[null,"S",null,null,15,null,"S",null,null,15,null,"S",null,null,15,null,"S","CP","SB8",15,null,"S","Ad16","Ad16",15,null,"S","AD0","SD0",15,null,"S","SE8","RW",15,null,"S",null,null,15,null,"S",null,null,15,null,"S","REG-5.1v",null,15,null,"S",null,null,15]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}